#MicroXplorer Configuration settings - do not modify
CAD.formats=
CAD.pinconfig=
CAD.provider=
CORTEX_M7.CPU_DCache=Enabled
CORTEX_M7.CPU_ICache=Enabled
CORTEX_M7.IPParameters=default_mode_Activation,CPU_ICache,CPU_DCache
CORTEX_M7.default_mode_Activation=1
Dma.Request0=SPI4_TX
Dma.RequestsNb=1
Dma.SPI4_TX.0.Direction=DMA_MEMORY_TO_PERIPH
Dma.SPI4_TX.0.EventEnable=DISABLE
Dma.SPI4_TX.0.FIFOMode=DMA_FIFOMODE_DISABLE
Dma.SPI4_TX.0.Instance=DMA1_Stream0
Dma.SPI4_TX.0.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.SPI4_TX.0.MemInc=DMA_MINC_ENABLE
Dma.SPI4_TX.0.Mode=DMA_NORMAL
Dma.SPI4_TX.0.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.SPI4_TX.0.PeriphInc=DMA_PINC_DISABLE
Dma.SPI4_TX.0.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.SPI4_TX.0.Priority=DMA_PRIORITY_LOW
Dma.SPI4_TX.0.RequestNumber=1
Dma.SPI4_TX.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,FIFOMode,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.SPI4_TX.0.SignalID=NONE
Dma.SPI4_TX.0.SyncEnable=DISABLE
Dma.SPI4_TX.0.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.SPI4_TX.0.SyncRequestNumber=1
Dma.SPI4_TX.0.SyncSignalID=NONE
File.Version=6
GPIO.groupedBy=Group By Peripherals
KeepUserPlacement=false
MMTAppRegionsCount=0
MMTConfigApplied=false
Mcu.CPN=STM32H723ZET6
Mcu.Family=STM32H7
Mcu.IP0=CORTEX_M7
Mcu.IP1=DEBUG
Mcu.IP2=DMA
Mcu.IP3=MEMORYMAP
Mcu.IP4=NVIC
Mcu.IP5=RCC
Mcu.IP6=RTC
Mcu.IP7=SDMMC1
Mcu.IP8=SPI4
Mcu.IP9=SYS
Mcu.IPNb=10
Mcu.Name=STM32H723ZETx
Mcu.Package=LQFP144
Mcu.Pin0=PE6
Mcu.Pin1=PC14-OSC32_IN
Mcu.Pin10=PC8
Mcu.Pin11=PC9
Mcu.Pin12=PA8
Mcu.Pin13=PA13(JTMS/SWDIO)
Mcu.Pin14=PA14(JTCK/SWCLK)
Mcu.Pin15=PC10
Mcu.Pin16=PC11
Mcu.Pin17=PC12
Mcu.Pin18=PD2
Mcu.Pin19=PD7
Mcu.Pin2=PC15-OSC32_OUT
Mcu.Pin20=PG9
Mcu.Pin21=PG10
Mcu.Pin22=PG11
Mcu.Pin23=PG12
Mcu.Pin24=PG13
Mcu.Pin25=VP_RTC_VS_RTC_Activate
Mcu.Pin26=VP_SYS_VS_tim7
Mcu.Pin27=VP_MEMORYMAP_VS_MEMORYMAP
Mcu.Pin28=VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_RTOSJjThreadX_6.4.0_3.3.0
Mcu.Pin29=VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjFileX_6.4.0_3.3.0
Mcu.Pin3=PH0-OSC_IN
Mcu.Pin30=VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjInterfaces_3.3.0_3.3.0
Mcu.Pin4=PH1-OSC_OUT
Mcu.Pin5=PE11
Mcu.Pin6=PE12
Mcu.Pin7=PE13
Mcu.Pin8=PE14
Mcu.Pin9=PE15
Mcu.PinsNb=31
Mcu.ThirdParty0=STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0
Mcu.ThirdPartyNb=1
Mcu.UserConstants=
Mcu.UserName=STM32H723ZETx
MxCube.Version=6.13.0
MxDb.Version=DB.6.0.130
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.DMA1_Stream0_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SDMMC1_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true\:true
NVIC.SPI4_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:true\:false
NVIC.TIM7_IRQn=true\:15\:0\:false\:false\:true\:false\:false\:true\:true
NVIC.TimeBase=TIM7_IRQn
NVIC.TimeBaseIP=TIM7
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false\:false
PA13(JTMS/SWDIO).Mode=Serial_Wire
PA13(JTMS/SWDIO).Signal=DEBUG_JTMS-SWDIO
PA14(JTCK/SWCLK).Mode=Serial_Wire
PA14(JTCK/SWCLK).Signal=DEBUG_JTCK-SWCLK
PA8.GPIOParameters=GPIO_PuPd,GPIO_Label
PA8.GPIO_Label=SD_DETECT
PA8.GPIO_PuPd=GPIO_PULLDOWN
PA8.Locked=true
PA8.Signal=GPIO_Input
PC10.Mode=SD_4_bits_Wide_bus
PC10.Signal=SDMMC1_D2
PC11.Mode=SD_4_bits_Wide_bus
PC11.Signal=SDMMC1_D3
PC12.Mode=SD_4_bits_Wide_bus
PC12.Signal=SDMMC1_CK
PC14-OSC32_IN.Mode=LSE-External-Oscillator
PC14-OSC32_IN.Signal=RCC_OSC32_IN
PC15-OSC32_OUT.Mode=LSE-External-Oscillator
PC15-OSC32_OUT.Signal=RCC_OSC32_OUT
PC8.Locked=true
PC8.Mode=SD_4_bits_Wide_bus
PC8.Signal=SDMMC1_D0
PC9.Mode=SD_4_bits_Wide_bus
PC9.Signal=SDMMC1_D1
PD2.Mode=SD_4_bits_Wide_bus
PD2.Signal=SDMMC1_CMD
PD7.GPIOParameters=GPIO_Label
PD7.GPIO_Label=OUTPUT_ON_LED
PD7.Locked=true
PD7.Signal=GPIO_Output
PE11.GPIOParameters=GPIO_Label
PE11.GPIO_Label=SPI4_NSS_DISPLAY
PE11.Locked=true
PE11.Mode=NSS_Signal_Hard_Output
PE11.Signal=SPI4_NSS
PE12.GPIOParameters=GPIO_Label
PE12.GPIO_Label=SPI4_SCK_DISPLAY
PE12.Locked=true
PE12.Mode=Simplex_Bidirectional_Master
PE12.Signal=SPI4_SCK
PE13.GPIOParameters=GPIO_Label
PE13.GPIO_Label=PWM_DISPLAY_LIGHT
PE13.Locked=true
PE13.Signal=GPIO_Output
PE14.GPIOParameters=GPIO_Label
PE14.GPIO_Label=SPI4_MOSI_DISPLAY
PE14.Locked=true
PE14.Mode=Simplex_Bidirectional_Master
PE14.Signal=SPI4_MOSI
PE15.GPIOParameters=PinState,GPIO_Label
PE15.GPIO_Label=RST_DISPLAY
PE15.Locked=true
PE15.PinState=GPIO_PIN_RESET
PE15.Signal=GPIO_Output
PE6.GPIOParameters=GPIO_Label
PE6.GPIO_Label=TX1_LED
PE6.Locked=true
PE6.Signal=GPIO_Output
PG10.GPIOParameters=GPIO_Label
PG10.GPIO_Label=CHARGE_LED
PG10.Locked=true
PG10.Signal=GPIO_Output
PG11.GPIOParameters=GPIO_Label
PG11.GPIO_Label=RX2_LED
PG11.Locked=true
PG11.Signal=GPIO_Output
PG12.GPIOParameters=GPIO_Label
PG12.GPIO_Label=RX1_LED
PG12.Locked=true
PG12.Signal=GPIO_Output
PG13.GPIOParameters=GPIO_Label
PG13.GPIO_Label=TX2_LED
PG13.Locked=true
PG13.Signal=GPIO_Output
PG9.GPIOParameters=GPIO_Label
PG9.GPIO_Label=ERROR_LED
PG9.Locked=true
PG9.Signal=GPIO_Output
PH0-OSC_IN.Mode=HSE-External-Oscillator
PH0-OSC_IN.Signal=RCC_OSC_IN
PH1-OSC_OUT.Mode=HSE-External-Oscillator
PH1-OSC_OUT.Signal=RCC_OSC_OUT
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32H723ZETx
ProjectManager.FirmwarePackage=STM32Cube FW_H7 V1.12.0
ProjectManager.FreePins=true
ProjectManager.HalAssertFull=true
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=charger.ioc
ProjectManager.ProjectName=charger
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_DMA_Init-DMA-false-HAL-true,4-MX_RTC_Init-RTC-false-HAL-true,5-MX_SPI4_Init-SPI4-false-HAL-true,6-MX_SDMMC1_SD_Init-SDMMC1-false-HAL-true,0-MX_CORTEX_M7_Init-CORTEX_M7-false-HAL-true
RCC.ADCFreq_Value=166666666.66666666
RCC.AHB12Freq_Value=100000000
RCC.AHB4Freq_Value=100000000
RCC.APB1Freq_Value=100000000
RCC.APB2Freq_Value=100000000
RCC.APB3Freq_Value=100000000
RCC.APB4Freq_Value=100000000
RCC.AXIClockFreq_Value=100000000
RCC.CECFreq_Value=32000
RCC.CKPERFreq_Value=64000000
RCC.CortexFreq_Value=100000000
RCC.CpuClockFreq_Value=100000000
RCC.D1CPREFreq_Value=100000000
RCC.DFSDMACLkFreq_Value=50000000
RCC.DFSDMFreq_Value=100000000
RCC.DIVM1=5
RCC.DIVM2=3
RCC.DIVM3=1
RCC.DIVN1=40
RCC.DIVN2=40
RCC.DIVN3=4
RCC.DIVP1Freq_Value=100000000
RCC.DIVP2Freq_Value=166666666.66666666
RCC.DIVP3Freq_Value=50000000
RCC.DIVQ1=4
RCC.DIVQ1Freq_Value=50000000
RCC.DIVQ2=11
RCC.DIVQ2Freq_Value=30303030.3030303
RCC.DIVQ3Freq_Value=50000000
RCC.DIVR1Freq_Value=100000000
RCC.DIVR2=10
RCC.DIVR2Freq_Value=33333333.333333332
RCC.DIVR3Freq_Value=50000000
RCC.FDCANFreq_Value=50000000
RCC.FMCFreq_Value=100000000
RCC.FamilyName=M
RCC.HCLK3ClockFreq_Value=100000000
RCC.HCLKFreq_Value=100000000
RCC.I2C123Freq_Value=100000000
RCC.I2C4Freq_Value=100000000
RCC.IPParameters=ADCFreq_Value,AHB12Freq_Value,AHB4Freq_Value,APB1Freq_Value,APB2Freq_Value,APB3Freq_Value,APB4Freq_Value,AXIClockFreq_Value,CECFreq_Value,CKPERFreq_Value,CortexFreq_Value,CpuClockFreq_Value,D1CPREFreq_Value,DFSDMACLkFreq_Value,DFSDMFreq_Value,DIVM1,DIVM2,DIVM3,DIVN1,DIVN2,DIVN3,DIVP1Freq_Value,DIVP2Freq_Value,DIVP3Freq_Value,DIVQ1,DIVQ1Freq_Value,DIVQ2,DIVQ2Freq_Value,DIVQ3Freq_Value,DIVR1Freq_Value,DIVR2,DIVR2Freq_Value,DIVR3Freq_Value,FDCANFreq_Value,FMCFreq_Value,FamilyName,HCLK3ClockFreq_Value,HCLKFreq_Value,I2C123Freq_Value,I2C4Freq_Value,LPTIM1Freq_Value,LPTIM2Freq_Value,LPTIM345Freq_Value,LPUART1Freq_Value,LTDCFreq_Value,MCO1PinFreq_Value,MCO2PinFreq_Value,PLL2FRACN,PLLFRACN,PLLSourceVirtual,QSPIFreq_Value,RNGFreq_Value,RTCClockSelection,RTCFreq_Value,SAI1Freq_Value,SAI4AFreq_Value,SAI4BFreq_Value,SDMMCFreq_Value,SPDIFRXFreq_Value,SPI123Freq_Value,SPI45Freq_Value,SPI6Freq_Value,SWPMI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,Spi45ClockSelection,Tim1OutputFreq_Value,Tim2OutputFreq_Value,TraceFreq_Value,USART16Freq_Value,USART234578Freq_Value,USBFreq_Value,VCO1OutputFreq_Value,VCO2OutputFreq_Value,VCO3OutputFreq_Value,VCOInput1Freq_Value,VCOInput2Freq_Value,VCOInput3Freq_Value
RCC.LPTIM1Freq_Value=100000000
RCC.LPTIM2Freq_Value=100000000
RCC.LPTIM345Freq_Value=100000000
RCC.LPUART1Freq_Value=100000000
RCC.LTDCFreq_Value=50000000
RCC.MCO1PinFreq_Value=64000000
RCC.MCO2PinFreq_Value=100000000
RCC.PLL2FRACN=0
RCC.PLLFRACN=0
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.QSPIFreq_Value=100000000
RCC.RNGFreq_Value=48000000
RCC.RTCClockSelection=RCC_RTCCLKSOURCE_LSE
RCC.RTCFreq_Value=32768
RCC.SAI1Freq_Value=50000000
RCC.SAI4AFreq_Value=50000000
RCC.SAI4BFreq_Value=50000000
RCC.SDMMCFreq_Value=50000000
RCC.SPDIFRXFreq_Value=50000000
RCC.SPI123Freq_Value=50000000
RCC.SPI45Freq_Value=25000000
RCC.SPI6Freq_Value=100000000
RCC.SWPMI1Freq_Value=100000000
RCC.SYSCLKFreq_VALUE=100000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.Spi45ClockSelection=RCC_SPI45CLKSOURCE_HSE
RCC.Tim1OutputFreq_Value=100000000
RCC.Tim2OutputFreq_Value=100000000
RCC.TraceFreq_Value=100000000
RCC.USART16Freq_Value=100000000
RCC.USART234578Freq_Value=100000000
RCC.USBFreq_Value=50000000
RCC.VCO1OutputFreq_Value=200000000
RCC.VCO2OutputFreq_Value=333333333.3333333
RCC.VCO3OutputFreq_Value=100000000
RCC.VCOInput1Freq_Value=5000000
RCC.VCOInput2Freq_Value=8333333.333333333
RCC.VCOInput3Freq_Value=25000000
SDMMC1.ClockPowerSave=SDMMC_CLOCK_POWER_SAVE_ENABLE
SDMMC1.HardwareFlowControl=SDMMC_HARDWARE_FLOW_CONTROL_ENABLE
SDMMC1.IPParameters=ClockPowerSave,HardwareFlowControl
SPI4.BaudRatePrescaler=SPI_BAUDRATEPRESCALER_4
SPI4.CalculateBaudRate=6.25 MBits/s
SPI4.DataSize=SPI_DATASIZE_9BIT
SPI4.Direction=SPI_DIRECTION_1LINE
SPI4.IPParameters=VirtualType,Mode,Direction,CalculateBaudRate,VirtualNSS,DataSize,BaudRatePrescaler
SPI4.Mode=SPI_MODE_MASTER
SPI4.VirtualNSS=VM_NSSHARD
SPI4.VirtualType=VM_MASTER
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FX_APP_MEM_POOL_SIZE=8192
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FX_DRIVER_SD_INIT=0
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FX_ENABLE_EXFAT=1
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FX_ENABLE_FAULT_TOLERANT=1
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FX_FAULT_TOLERANT=1
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FX_FAULT_TOLERANT_DATA=1
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FileOoSystemJjFileX_Checked=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FileOoSystemJjInterfaces_Checked=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.FileXCcFileOoSystemJjFileXJjCore=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.IPParameters=TX_APP_MEM_POOL_SIZE,FX_APP_MEM_POOL_SIZE,TX_APP_GENERATE_INIT_CODE,TX_APP_CREATION,TX_ENABLE_STACK_CHECKING,TX_NO_FILEX_POINTER,TX_LOW_POWER,FX_ENABLE_EXFAT,FX_ENABLE_FAULT_TOLERANT,FX_FAULT_TOLERANT,FX_FAULT_TOLERANT_DATA,FX_DRIVER_SD_INIT,ThreadXCcRTOSJjThreadXJjCore,ThreadXCcRTOSJjThreadXJjLowOoPowerOosupport,FileXCcFileOoSystemJjFileXJjCore,InterfacesCcFileOoSystemJjFileXOoSDOointerface,TX_TIMER_TICKS_PER_SECOND
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.InterfacesCcFileOoSystemJjFileXOoSDOointerface=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.RTOSJjThreadX_Checked=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.TX_APP_CREATION=0
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.TX_APP_GENERATE_INIT_CODE=false
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.TX_APP_MEM_POOL_SIZE=8192
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.TX_ENABLE_STACK_CHECKING=1
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.TX_LOW_POWER=1
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.TX_NO_FILEX_POINTER=1
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.TX_TIMER_TICKS_PER_SECOND=1000
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.ThreadXCcRTOSJjThreadXJjCore=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0.ThreadXCcRTOSJjThreadXJjLowOoPowerOosupport=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0_IsAnAzureRtosMw=true
STMicroelectronics.X-CUBE-AZRTOS-H7.3.3.0_SwParameter=InterfacesCcFileOoSystemJjFileXOoSDOointerface\:true;ThreadXCcRTOSJjThreadXJjLowOoPowerOosupport\:true;FileXCcFileOoSystemJjFileXJjCore\:true;ThreadXCcRTOSJjThreadXJjCore\:true;
VP_MEMORYMAP_VS_MEMORYMAP.Mode=CurAppReg
VP_MEMORYMAP_VS_MEMORYMAP.Signal=MEMORYMAP_VS_MEMORYMAP
VP_RTC_VS_RTC_Activate.Mode=RTC_Enabled
VP_RTC_VS_RTC_Activate.Signal=RTC_VS_RTC_Activate
VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjFileX_6.4.0_3.3.0.Mode=FileOoSystemJjFileX
VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjFileX_6.4.0_3.3.0.Signal=STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjFileX_6.4.0_3.3.0
VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjInterfaces_3.3.0_3.3.0.Mode=FileOoSystemJjInterfaces
VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjInterfaces_3.3.0_3.3.0.Signal=STMicroelectronics.X-CUBE-AZRTOS-H7_VS_FileOoSystemJjInterfaces_3.3.0_3.3.0
VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_RTOSJjThreadX_6.4.0_3.3.0.Mode=RTOSJjThreadX
VP_STMicroelectronics.X-CUBE-AZRTOS-H7_VS_RTOSJjThreadX_6.4.0_3.3.0.Signal=STMicroelectronics.X-CUBE-AZRTOS-H7_VS_RTOSJjThreadX_6.4.0_3.3.0
VP_SYS_VS_tim7.Mode=TIM7
VP_SYS_VS_tim7.Signal=SYS_VS_tim7
board=custom
