(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.74)
		(legacy_teardrops no)
	)
	(paper "A3" portrait)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user "User.2 -Bemaßung")
		(43 "User.3" user "User.3 - Heatsink")
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Red")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.07)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.58)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.07)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 100 120)
		(grid_origin 173 120)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "BAT+CONTROLED")
	(net 3 "/chargeControl/SWITCH_OUT")
	(net 4 "/B+Terminal")
	(net 5 "unconnected-(H1-Pad1)")
	(net 6 "unconnected-(H3-Pad1)")
	(net 7 "unconnected-(H5-Pad1)")
	(net 8 "unconnected-(H9-Pad1)")
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
		(layer "F.Cu")
		(uuid "1ec47d88-b708-4c37-91f7-170794f14407")
		(at 243 295)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H5"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(uuid "acbc81eb-de27-42b8-8361-8eac01de90d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(uuid "d72d3135-a218-410a-8059-69abf0bfbc99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7bc21e47-e430-4d0a-b938-e34d3f0002c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1bf06e86-5565-4062-8786-f2a69a6f19b1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9b7cff28-a398-492c-9dea-e726c5d62f70")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3ea532d1-fd1d-413c-ae00-4116b06e70cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "64dfcd3b-271d-4214-9f53-ab4774b6d514")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dfbe0be9-ea9f-46fa-9b65-70d63e73b7b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a841e4a-713b-4a43-abc2-8e349ce3dc89")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0bb36590-58f1-4361-8564-fd18d8528ffe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(path "/33dcd0ca-d890-497c-ad50-9a6e3a10ee6a")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.9 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "6e4478f8-5f22-4cba-afef-14c1e25ef43e")
		)
		(fp_circle
			(center 0 0)
			(end 2.15 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "040613bb-3ca5-4902-a81c-158e06f8bed0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ac8e4b0e-dbba-4749-8fdd-d9714b44b1f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(H5-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
			(uuid "6e32e292-2d52-46f0-804d-221244910a41")
		)
		(embedded_fonts no)
	)
	(footprint "myWürthSHFU:WP-SHFU_7461098_HAL"
		(layer "F.Cu")
		(uuid "37f9dadd-4df2-4bc8-8810-c3fa3706f53f")
		(at 204 165)
		(descr "WP-SHFU External thread, full plain\nDrill hole specification for HAL\nThread M6 , 25pins\nMax Height = 15.5mm")
		(property "Reference" "J16"
			(at 0 8.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "eeb26d63-cce6-4040-8dbe-d8f004bea3ee")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify bottom)
			)
		)
		(property "Value" "Würth RedCube"
			(at -3.5 8.8 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "d3e479d1-cc0b-499c-9081-1d348c769dc3")
			(effects
				(font
					(size 1.1684 1.1684)
					(thickness 0.1016)
				)
				(justify left bottom)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "366ea1be-ee6b-427b-8ed3-395be56da1ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M6 PRESS FIT 250A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d8bb14f2-5b8a-4f46-aee0-8460b622e3d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "CON521"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3edfe65-5d46-4071-ad91-73cd41f1cd79")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "7461098"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "53d70083-8fe2-40f3-b31a-24e1492082d1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5e469602-d93f-4741-a06e-18f4a8696c0c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4b980409-687b-46ac-97c6-b10d1ec98c6a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "Würth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "57fdaea3-9523-4e02-8c63-534b43adb17d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7743c3e0-bc4f-4bd6-83a3-3b4f931dc780")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c935d01-0dcb-4ff9-8a23-553ab0e238a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4432c41e-3e50-4a1a-8643-482bd9b1a618")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/cb274230-c4d1-40d2-a738-3d4c8cbe3cb6")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -6.6 -6.6)
			(end 6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "06e12ac9-7a13-4858-a88e-e429470a4f8d")
		)
		(fp_line
			(start -6.6 6.6)
			(end -6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90d2101d-863e-4232-b116-96920c5ce349")
		)
		(fp_line
			(start 6.6 -6.6)
			(end 6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e253098-81ac-48cc-95f8-c0ab6361588b")
		)
		(fp_line
			(start 6.6 6.6)
			(end -6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0905974c-309b-49d0-99b1-08322d968b78")
		)
		(fp_poly
			(pts
				(xy 6.85 6.85) (xy -6.85 6.85) (xy -6.85 -6.85) (xy 6.85 -6.85)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.CrtYd")
			(uuid "692cc78f-1ae4-48ba-843c-97a224be24db")
		)
		(fp_line
			(start -6.5 -6.5)
			(end 6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a332b3ac-35ae-4c90-8fbe-87de0ffdb7ce")
		)
		(fp_line
			(start -6.5 6.5)
			(end -6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c2e0252-164c-41ae-a1ba-5c17d1fa285a")
		)
		(fp_line
			(start 6.5 -6.5)
			(end 6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2413d5ee-dd57-40d8-84e8-70cb70e2d58e")
		)
		(fp_line
			(start 6.5 6.5)
			(end -6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f71feb27-f2cd-4b5a-a6a5-e2b1101eaacb")
		)
		(pad "1" thru_hole circle
			(at -5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "17c8b9cd-67d6-4613-93aa-a3335c3e57af")
		)
		(pad "1" thru_hole circle
			(at -5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "7b2e25a6-a07c-4079-bd73-ee247ed52b25")
		)
		(pad "1" thru_hole circle
			(at -5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "266136e7-ce21-41fa-98a7-ca346323db56")
		)
		(pad "1" thru_hole circle
			(at -5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "8f2cc214-8cdc-4335-ab97-8062346e89bd")
		)
		(pad "1" thru_hole circle
			(at -5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "25d24185-552d-4f5f-a3c9-c9d9258bdd02")
		)
		(pad "1" thru_hole circle
			(at -2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "d99c99ad-b6f7-4764-bff7-cf43f9448f07")
		)
		(pad "1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "57f281e8-e188-431b-8e0c-0afca6cfb278")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "375ebcec-cb87-4484-91a7-9dc271605a95")
		)
		(pad "1" thru_hole circle
			(at -2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "cad44a88-6538-4164-b5b9-d3dec63c183a")
		)
		(pad "1" thru_hole circle
			(at -2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "477e8173-7a8d-4931-a52c-1334b5ee2bc7")
		)
		(pad "1" thru_hole circle
			(at 0 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "3dbe1ceb-3c50-4a78-a2b5-67394363bfd0")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "d1bfae20-eefb-45cb-97f9-3fd3a0cf385c")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "7bcc2920-e83c-4855-9e34-924979156724")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "02760036-f785-4416-a2d6-14543eb8fcd5")
		)
		(pad "1" thru_hole circle
			(at 0 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "19d5c4f8-cd48-4fac-9ed4-5886b78761cf")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "e813ab69-9c1d-45ca-9c86-15f9506ae61b")
		)
		(pad "1" thru_hole circle
			(at 2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "1db85049-47d1-4bd4-a4c6-a6a8951b9a53")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "db71dd8c-bac6-4ffe-a8bc-856fa4eebc78")
		)
		(pad "1" thru_hole circle
			(at 2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "44e8ce56-ec62-4233-a8aa-a56b7621b197")
		)
		(pad "1" thru_hole circle
			(at 2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c9b61ad4-12bc-4455-afd7-e97b716f9d1c")
		)
		(pad "1" thru_hole circle
			(at 5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b8b105e9-bbe0-4187-858d-e9d5d68bcd14")
		)
		(pad "1" thru_hole circle
			(at 5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "65d36e10-064a-42db-ad66-d811550e1b86")
		)
		(pad "1" thru_hole circle
			(at 5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "7a72f581-7431-4600-8084-366d3058dbb5")
		)
		(pad "1" thru_hole circle
			(at 5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "f5ed0229-b390-4de2-9e13-c446165723a8")
		)
		(pad "1" thru_hole circle
			(at 5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "797428e1-9b0b-4005-af8f-a865e7951e37")
		)
		(embedded_fonts no)
		(model "D:/projekte/Kicad/8.0/3dmodels/würth_shfu_redcube_einpressbolzen/7461098.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "myWürthSHFU:WP-SHFU_7461098_HAL"
		(layer "F.Cu")
		(uuid "38d28ba7-524f-4ab5-9ac1-8ed8c4c251ab")
		(at 204 245)
		(descr "WP-SHFU External thread, full plain\nDrill hole specification for HAL\nThread M6 , 25pins\nMax Height = 15.5mm")
		(property "Reference" "J15"
			(at 0 -7.6 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "6369455e-a1fc-4e02-9398-b550c6857dfa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify bottom)
			)
		)
		(property "Value" "Würth RedCube"
			(at -3.5 8.8 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "62962bdb-f630-462f-9f09-bda44250d2d4")
			(effects
				(font
					(size 1.1684 1.1684)
					(thickness 0.1016)
				)
				(justify left bottom)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3b4f2a53-3822-4be7-95b4-f0f0e389b477")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M6 PRESS FIT 250A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7b1eb072-dd8f-412b-bd55-ad3e2abff874")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "CON521"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dfd285f8-fb21-4f87-8911-22430aebb539")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "7461098"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f684c16-b345-4ff9-89b3-fa6a47ed2b62")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9aba5fca-1577-4b81-b6fe-85c13f0840e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3590cfc7-e958-44fa-b727-eef8aa3ce5a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "Würth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "57f7f8f1-6030-41b3-9719-7b31c407051a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0307545c-0a09-4915-a7d3-9b5a812a03f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "166582c4-8294-43f4-9472-8dbf458eace8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "44bc7782-1adb-4e64-8a1c-a454b11676b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/32c75c69-863f-4bd5-99ba-a833ca4d9182")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -6.6 -6.6)
			(end 6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8c6c997-c8c0-4016-8d3e-968abeb2927d")
		)
		(fp_line
			(start -6.6 6.6)
			(end -6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bdb0df7d-7932-46c7-8d60-916de939c0a1")
		)
		(fp_line
			(start 6.6 -6.6)
			(end 6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83772658-337b-402a-8eb8-750d6f004be9")
		)
		(fp_line
			(start 6.6 6.6)
			(end -6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14e85fdd-0ab9-40ad-a5f5-71053c548bbf")
		)
		(fp_poly
			(pts
				(xy 6.85 6.85) (xy -6.85 6.85) (xy -6.85 -6.85) (xy 6.85 -6.85)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.CrtYd")
			(uuid "0fae5cd2-f904-4b34-84c7-8bf17c470e58")
		)
		(fp_line
			(start -6.5 -6.5)
			(end 6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "afa91327-57a8-493c-9f69-0cb3484d3e28")
		)
		(fp_line
			(start -6.5 6.5)
			(end -6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac1797b9-ff54-49fa-afcb-4ccdfb28e430")
		)
		(fp_line
			(start 6.5 -6.5)
			(end 6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a891e6e0-2334-430d-9584-9e0e62c01da9")
		)
		(fp_line
			(start 6.5 6.5)
			(end -6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4aaa94cb-5054-4ec4-96f7-c54e16c13360")
		)
		(pad "1" thru_hole circle
			(at -5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "87f05ace-5acc-49fd-b987-dc1508c70ad5")
		)
		(pad "1" thru_hole circle
			(at -5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "246dcdf2-aee6-4fd9-8c2f-d9a6489d41a1")
		)
		(pad "1" thru_hole circle
			(at -5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "feb30ef1-8ffb-47b0-a5ff-5a23ed03b7d5")
		)
		(pad "1" thru_hole circle
			(at -5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c2a1012f-0136-4581-83eb-b8d16744a904")
		)
		(pad "1" thru_hole circle
			(at -5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "33f1c354-ca0b-4262-99ee-7979e1fea748")
		)
		(pad "1" thru_hole circle
			(at -2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c9c91225-c2a8-4ff7-bc91-2c6189e636ac")
		)
		(pad "1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "d73253f9-4df6-48dd-8b5f-244b3a4e66f2")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "e2666bf2-0e91-47f2-899a-7f84b54f6d40")
		)
		(pad "1" thru_hole circle
			(at -2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "573abc5e-6f4a-4b16-ab14-dcb618737807")
		)
		(pad "1" thru_hole circle
			(at -2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "278b8595-3006-4b6f-af2d-0b6966c0d5e8")
		)
		(pad "1" thru_hole circle
			(at 0 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "091b1898-a739-42be-ac8f-9c0100f13fa0")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c80f6c82-c7bc-4cb9-a443-9e838789a776")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "5c7884f0-dc01-48b3-b82b-3243f652b76e")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "3aaa804d-5289-444b-bbd4-13471b904ff7")
		)
		(pad "1" thru_hole circle
			(at 0 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "64c4f918-b227-4fae-bd63-bef1615dfc55")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "9ee27995-905a-457f-8cde-8633820c6e97")
		)
		(pad "1" thru_hole circle
			(at 2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "1257170e-34f4-4f1f-b585-620fd8a6a3a8")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "64c91559-d7d7-4d8e-b883-6722d67e64f7")
		)
		(pad "1" thru_hole circle
			(at 2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "592dea1b-6e03-4843-b800-66d2bd1eef48")
		)
		(pad "1" thru_hole circle
			(at 2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "0abdb90d-1fc9-4648-b075-e3c60f46d291")
		)
		(pad "1" thru_hole circle
			(at 5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "bcb53a7a-a4f0-49d5-ae15-c8278badf1e6")
		)
		(pad "1" thru_hole circle
			(at 5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "5f6af950-0a0f-4566-b1dc-c43f50f8b0b0")
		)
		(pad "1" thru_hole circle
			(at 5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "5685c693-2288-4d44-ac95-6d9a3061798d")
		)
		(pad "1" thru_hole circle
			(at 5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "96e140d5-e436-418b-8426-5514cd461bb0")
		)
		(pad "1" thru_hole circle
			(at 5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "BAT+CONTROLED")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b60f3ad8-0f42-43a9-80ef-85992fd614a1")
		)
		(embedded_fonts no)
		(model "D:/projekte/Kicad/8.0/3dmodels/würth_shfu_redcube_einpressbolzen/7461098.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "myWürthSHFU:WP-SHFU_7461098_HAL_gewinkelt"
		(layer "F.Cu")
		(uuid "3b7fefe3-d14f-4a9e-90f0-d591868ebed2")
		(at 142 129.25)
		(descr "WP-SHFU External thread, full plain\nDrill hole specification for HAL\nThread M6 , 25pins\nMax Height = 15.5mm")
		(property "Reference" "J1"
			(at 0 -7.6 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a21f82b2-f676-4599-96f1-d8870d3b6ac6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify bottom)
			)
		)
		(property "Value" "Würth RedCube"
			(at -3.5 8.8 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "64230163-2374-4dbf-8908-e9420b208051")
			(effects
				(font
					(size 1.1684 1.1684)
					(thickness 0.1016)
				)
				(justify left bottom)
			)
		)
		(property "Datasheet" "https://www.we-online.com/de/components/products/REDCUBE_PRESS-FIT_RIGHT_ANGLED_EDGE_POSITION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7a02816-f991-41ce-8447-f75290772e16")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M6 PRESS FIT 250A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e95b5d91-bd55-43ff-acd1-93934e244239")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "CON529"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "698fed63-0f46-4287-a4da-5a17c907cd99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "74622106"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5654d78b-f28e-4b91-a6de-88981c0aedf6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "739a9b5e-af9a-4922-a165-8558c79d62ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "971bddf7-2883-4064-a552-268f8240379b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "Würth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "04cd1a3c-2f8e-496b-a450-18ea1768c81b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "992986d2-9143-40bc-aa30-f6eb220c5aec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "36e63314-2f3a-47c6-b9d7-7e257d81ad5c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f5d064ab-2272-409d-9890-03645a32c28f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/8c864aab-b36a-433f-a345-2eacdf7e8e48")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -6.6 -6.6)
			(end 6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd97cdb6-d57b-40f0-bed6-723e9e289b64")
		)
		(fp_line
			(start -6.6 6.6)
			(end -6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47c6694f-9a5f-41c8-85e2-7c46dc3fd928")
		)
		(fp_line
			(start -6.5 -9.25)
			(end -6.5 3.75)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "dc7e6c89-68b7-4922-916e-b710d6f7dcd6")
		)
		(fp_line
			(start -6.5 3.75)
			(end 6.5 3.75)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "32917012-e8c6-4c68-9040-209ccf41df08")
		)
		(fp_line
			(start 6.5 -9.25)
			(end -6.5 -9.25)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "8a8403cb-9ae8-4d14-812d-a237ac73c3bf")
		)
		(fp_line
			(start 6.5 3.75)
			(end 6.5 -9.25)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "42e05f38-57a7-42f3-8a78-f64702bb89e9")
		)
		(fp_line
			(start 6.6 -6.6)
			(end 6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3252cca7-0907-477d-9636-c26d7231d646")
		)
		(fp_line
			(start 6.6 6.6)
			(end -6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a63722c-6d7f-4e8f-b061-862c2bc48c68")
		)
		(fp_poly
			(pts
				(xy 6.85 6.85) (xy -6.85 6.85) (xy -6.85 -6.85) (xy 6.85 -6.85)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.CrtYd")
			(uuid "7beeb530-62ce-4f5a-8a02-f76c9bf0f66d")
		)
		(fp_line
			(start -6.5 -6.5)
			(end 6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d18049a7-0207-43e8-a520-7cae62ed04e0")
		)
		(fp_line
			(start -6.5 6.5)
			(end -6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69ee079f-7ec2-4e12-94eb-d1d09c6f0c0c")
		)
		(fp_line
			(start 6.5 -6.5)
			(end 6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "006af42e-5d67-4ddc-9624-ae9f001011d2")
		)
		(fp_line
			(start 6.5 6.5)
			(end -6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cb14ab2-3bda-47ee-a32c-76cb8c8fda32")
		)
		(pad "1" thru_hole circle
			(at -5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "4bb5829c-546c-4569-aa8b-a69e51e700a3")
		)
		(pad "1" thru_hole circle
			(at -5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "aafbc843-17d4-44ad-a6d9-60f67afbd4f9")
		)
		(pad "1" thru_hole circle
			(at -5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "35027d35-cafa-4fbc-8a2f-6e1d98820ebc")
		)
		(pad "1" thru_hole circle
			(at -5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "637e38b8-155b-4581-8151-7e82598d008d")
		)
		(pad "1" thru_hole circle
			(at -5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "cba74cf0-4ec0-49a8-b115-cdd75f774c7a")
		)
		(pad "1" thru_hole circle
			(at -2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "8dc00d31-2b1b-4b13-bac1-59adf9fd0f4c")
		)
		(pad "1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "356aa8da-f0a2-4074-92dc-2202521bf593")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b84f3b8d-e36b-4fdb-8f70-5a6d50a9f5f6")
		)
		(pad "1" thru_hole circle
			(at -2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "78d546f6-8b74-41db-bc67-0f344e70c2c0")
		)
		(pad "1" thru_hole circle
			(at -2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "af068636-e607-475d-85f6-30da8963ebb2")
		)
		(pad "1" thru_hole circle
			(at 0 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "e078a617-3c1c-4c99-a2e3-a43cefba7340")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "867d14d1-a13e-4cbb-a8f0-14e29ca961a5")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "2a6ba24f-3e3f-4ea2-bb39-01b5816d0f97")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c76568e1-3d7c-4e5f-b8f2-1bfeeb6930e3")
		)
		(pad "1" thru_hole circle
			(at 0 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "99876c73-c9a8-42e5-b2fd-0781a00d2952")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "d94d643f-d155-41d8-9fa8-61d2511b2d00")
		)
		(pad "1" thru_hole circle
			(at 2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "56cb545d-3d8e-4ebd-a985-ab191cca4018")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "9b4d337e-701c-4099-a280-3d53ea1b9946")
		)
		(pad "1" thru_hole circle
			(at 2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "8a0928c1-542b-4866-90c0-16f9ea4641c8")
		)
		(pad "1" thru_hole circle
			(at 2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "992380fd-5646-4f9a-a495-18724cb126f1")
		)
		(pad "1" thru_hole circle
			(at 5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "041cec89-f5b0-43ab-9c07-9374e105126b")
		)
		(pad "1" thru_hole circle
			(at 5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "77f6ad28-0781-4c32-8d70-04842ead1b49")
		)
		(pad "1" thru_hole circle
			(at 5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "303b73aa-e43c-438b-afb0-e50afdcbc3d8")
		)
		(pad "1" thru_hole circle
			(at 5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "4f7f8cb5-9618-47b4-ab99-cf2d0711fecf")
		)
		(pad "1" thru_hole circle
			(at 5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c031b86e-d1c8-4b9b-a1ca-e972f3edea1f")
		)
		(embedded_fonts no)
		(model "D:/projekte/Kicad/8.0/3dmodels/würth_shfu_redcube_einpressbolzen/74622106.stp"
			(offset
				(xyz 0 2.54 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "myHoles:printer_mounting_holes_1mm"
		(layer "F.Cu")
		(uuid "477a4379-c48e-448f-9d5f-a5a9eb423762")
		(at 110.5 294.75)
		(property "Reference" "H2"
			(at 0 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "c5ed5a3b-0ed3-4fad-a00e-605458815de4")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "PastPrinterHole"
			(at 0 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "1d5cbb68-b23e-4f78-97d9-42ca4623b2c2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f096caf4-1583-4f16-a9e4-fec1bc9c3bfc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Past Printer Hole"
			(at 0 7.62 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4ed8b08-ed7e-4ff5-9660-6e728c8aac6a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ddeef3e-f1c6-4ad0-839c-bb43d2a913dd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "677211d1-dba5-4695-8744-a39c2cb788d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd30db4c-87fc-4e36-8b50-3dc79cd787cb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "89f5a383-5ada-41f0-aa92-573a74802f0a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "da8a2082-886c-4134-aab0-0810201e4185")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5ba7fd75-4294-4a38-bd42-f3b125b9684a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/d2c5cdd4-6fd4-41f3-8e3c-923d5f4a91cc")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "9914a2db-6c3b-477e-97fe-9c28aed0925a")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "f1b93fdf-dea6-4d8d-98bc-c42a69ae9667")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "f808a361-b602-4709-8af5-07350651d65f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(uuid "9868b159-be9e-4794-933b-cb4bd7a31108")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
		(layer "F.Cu")
		(uuid "4ad5423b-70d1-447f-986f-cf00226ef168")
		(at 103 125)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H3"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(uuid "01fada7b-d20a-4adf-a78a-682f4b27e978")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(uuid "8ba7e4a7-f1e1-45b7-b24b-c97c0632843d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f3d8716-da91-4638-996e-75195aa05893")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5e2ed41-ccea-40ef-b4e7-522088ab264b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2c4d378-07e6-4764-af5b-8f7370bbbafd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a6d6c60-5fe4-421e-9e7d-04d3e142a368")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "41749be5-0b9a-490c-9727-435d42902493")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "94074146-c06f-4677-b100-385c87552399")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ffc317a-95e3-4a6b-be7e-474c852caec1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3a69f389-2d6f-40db-bbb4-386b6c3fe9f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(path "/b56f1633-d0b9-49e4-b1cd-5ea7110d3a65")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.9 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "5a50c798-c9cf-48ba-ab89-846ac03a993a")
		)
		(fp_circle
			(center 0 0)
			(end 2.15 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "1691160c-9887-48d2-b0c2-65f1ca121536")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d7b37df3-8a51-4256-8311-7cdb1958e90c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(H3-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
			(uuid "dff3debe-a0a4-4199-97c4-cc5ea6070cda")
		)
		(embedded_fonts no)
	)
	(footprint "myWürthSHFU:WP-SHFU_7461098_HAL"
		(locked yes)
		(layer "F.Cu")
		(uuid "5279abf7-1904-4dbe-ad66-3c0856f44083")
		(at 142 225)
		(descr "WP-SHFU External thread, full plain\nDrill hole specification for HAL\nThread M6 , 25pins\nMax Height = 15.5mm")
		(property "Reference" "J5"
			(at 0 -7.6 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "cdef8223-cfda-46e7-a31e-621941b40b51")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify bottom)
			)
		)
		(property "Value" "Würth RedCube"
			(at -3.5 8.8 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "1ed8d360-a0cd-4414-b292-04914b854037")
			(effects
				(font
					(size 1.1684 1.1684)
					(thickness 0.1016)
				)
				(justify left bottom)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b467e2e5-60f5-4785-9b82-b10dec9483d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M6 PRESS FIT 250A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "beb3f83d-3368-43b1-8c01-17675904d274")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "CON521"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cec601a8-2410-4777-9a20-f279ffb23ea6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "7461098"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "540d7181-8397-40bf-ac74-2e917a842fad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "24a27c04-a023-460a-a8e2-a99e12fa7a4b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "004b3a84-c904-4585-94c0-e4a158ab4ae8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "Würth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "857310de-a7e0-47b0-b9e9-d8282048da9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "148d4e7f-d418-4daa-ab60-a8ac3f72a156")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "86924a81-0430-4e9d-8698-b5871c361b78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a137f4b-dddf-42fd-9c02-386e8f6def4e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/9f866409-de60-4e97-86d5-eca7fac5e40b")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -6.6 -6.6)
			(end 6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f9c21fa-953a-4af9-bf9f-7506e023a796")
		)
		(fp_line
			(start -6.6 6.6)
			(end -6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37b3b3d7-3314-40c7-a902-d7d1fcbc38cd")
		)
		(fp_line
			(start 6.6 -6.6)
			(end 6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83141a5d-250a-44ad-a168-842370e14e80")
		)
		(fp_line
			(start 6.6 6.6)
			(end -6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "422b259f-01bc-4f94-b0e8-6b456fb7f686")
		)
		(fp_poly
			(pts
				(xy 6.85 6.85) (xy -6.85 6.85) (xy -6.85 -6.85) (xy 6.85 -6.85)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.CrtYd")
			(uuid "2dc6c176-581d-4430-95bf-17b1b621e158")
		)
		(fp_line
			(start -6.5 -6.5)
			(end 6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1be75e9-2995-4c9d-ad6d-d723dc1edc90")
		)
		(fp_line
			(start -6.5 6.5)
			(end -6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbf27ed8-d804-4939-adbd-084bc46dc85f")
		)
		(fp_line
			(start 6.5 -6.5)
			(end 6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0970c065-c48f-4424-afd5-070de0527186")
		)
		(fp_line
			(start 6.5 6.5)
			(end -6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e10117b-0ed2-4533-b6fa-009a23ebbed1")
		)
		(pad "1" thru_hole circle
			(at -5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "80fb9c12-a8b6-46c7-b8d1-6fb9a3a988d9")
		)
		(pad "1" thru_hole circle
			(at -5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "41995799-470b-4e9f-8623-523af0a8507a")
		)
		(pad "1" thru_hole circle
			(at -5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "d631833a-a88e-4252-b7ed-32ef430fe589")
		)
		(pad "1" thru_hole circle
			(at -5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "5adaf990-72d2-4f47-a069-a4fc7a3fd6a8")
		)
		(pad "1" thru_hole circle
			(at -5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "6bdda8e2-8745-4064-a3bc-f3dc44bc64ac")
		)
		(pad "1" thru_hole circle
			(at -2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "2e13a7c4-6617-4973-9a04-f2cdea15daed")
		)
		(pad "1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ed80d351-75df-4525-8cd8-bbe200d947bd")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "0394a087-739d-4cd5-9894-9cb62dbc596f")
		)
		(pad "1" thru_hole circle
			(at -2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "3d685c44-b9dc-47d0-9bd4-b3b147194db3")
		)
		(pad "1" thru_hole circle
			(at -2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "e10ee529-599d-4299-823b-0cbb6ce5ad41")
		)
		(pad "1" thru_hole circle
			(at 0 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "49227aab-6448-416a-88fc-61f72f472793")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "8cd68ee5-a01c-488e-bbc2-7986c9d82e02")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "cf7526a0-e105-43f2-9465-1bbc2308a8b3")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "bfa8049c-4285-4d17-8f84-6409e64dfd82")
		)
		(pad "1" thru_hole circle
			(at 0 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "020816e1-793c-4a08-ae01-cc814e4acf09")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "03274a4f-2dde-4bc5-bab6-8fe2f2c79d84")
		)
		(pad "1" thru_hole circle
			(at 2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "9f55f2fd-2785-4e2e-86d6-72a81c603933")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "6f7ae6f8-ea90-4d42-a356-50264ae718c5")
		)
		(pad "1" thru_hole circle
			(at 2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b3b7aff6-4f49-4a01-a369-c800c4764c36")
		)
		(pad "1" thru_hole circle
			(at 2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "1c15aece-113b-4678-9410-c5cba4c97842")
		)
		(pad "1" thru_hole circle
			(at 5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "e849b042-4a18-4d7c-bbda-7d11233d91c4")
		)
		(pad "1" thru_hole circle
			(at 5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c964d0fd-b99e-4b6f-b4e8-9cc934e7c28c")
		)
		(pad "1" thru_hole circle
			(at 5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "1c36613e-3ed6-40cb-a68f-98e40e420206")
		)
		(pad "1" thru_hole circle
			(at 5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "cb8afb2c-301e-451b-b32c-74abd8271a6a")
		)
		(pad "1" thru_hole circle
			(at 5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/chargeControl/SWITCH_OUT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "7160cd65-7550-40e9-8ea0-82984998f729")
		)
		(embedded_fonts no)
		(model "D:/projekte/Kicad/8.0/3dmodels/würth_shfu_redcube_einpressbolzen/7461098.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "F.Cu")
		(uuid "5ffb2df7-885b-4575-b3e6-6f47e5e6c0d1")
		(at 228 295)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID3"
			(at 0 -2.54 0)
			(layer "F.SilkS")
			(uuid "9bc8cba6-48ca-4db0-93e3-a439dcb9f4c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fiducial"
			(at 0 2.286 0)
			(layer "F.Fab")
			(uuid "d02cab08-8835-44c3-9cdd-66bc2c235d35")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6ac4e25-fd32-4d55-bcc1-f98ac0af221e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a6520b7c-2f3d-416c-ad1d-e862b442e283")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8170d350-957d-4c1d-ad85-bbd5a95ecb74")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5112c9d-6c96-460a-b2ed-1a6f7756bbfa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f9a0069-6f98-4576-ab1d-b96ba5f5a84b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4910d8a5-ddd5-44eb-a314-a61ee416b785")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bfb2d53e-432c-4d1b-aaaa-47ad286a4831")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b1a8816c-7a14-4042-b3f7-d05ca71771a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dc662c09-a29c-4b7a-a8d6-588875df190d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "968ddcaf-9e00-4090-92cd-4881f7e43d15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/d0236751-8fd6-4dfc-ba19-eb335c11a859")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "4526693e-fb94-4648-8e08-240c4cd5a6b8")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "85065bf8-12d8-42dc-9106-97a38c310f03")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d8d3f31d-8982-45c0-a040-6098fe07c062")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "3b1871a4-4910-4abe-8e02-ed64000081bc")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
		(layer "F.Cu")
		(uuid "619bca11-a17d-4c4a-8bcf-d19563f78b91")
		(at 243 125)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H9"
			(at 0 3.5 0)
			(layer "F.SilkS")
			(uuid "38c22ba8-80af-4bf0-914f-f4953b46ddbc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(uuid "87dc1f56-f23d-4e21-ad30-24df9e99d87b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4da329d5-d838-4d58-9859-ae972b694c33")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dcd89fa4-e42f-46f1-86cd-74f0e733bea7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6ae7b22-12a8-4324-9a51-91858d60f70d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a5675855-adef-4e92-829d-04f4a7653925")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa74398a-a35f-4fa9-a721-14c3787095da")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6e59b506-0fd8-46ee-a97f-0bba0da268ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68d378a4-d704-4dd4-a8e6-3dfed9c60023")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0f176c0a-3e6e-4c36-81f2-4d7e56a723a9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(path "/01ffa3c0-8f36-4205-a7d2-33118f82ae63")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.9 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "e56cc4a3-bb0b-4695-b006-67888d91b36f")
		)
		(fp_circle
			(center 0 0)
			(end 2.15 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "079b19b3-11bc-43b4-9b41-b16854395504")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "080c4159-d73a-4971-a13c-ae2d557b5849")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(H9-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
			(uuid "11641d12-6e3b-41dd-b377-7f99a55b0f79")
		)
		(embedded_fonts no)
	)
	(footprint "myHoles:printer_mounting_holes_1mm"
		(layer "F.Cu")
		(uuid "8b77cb70-e320-45ff-b4c3-ed83fde94006")
		(at 110.5 125)
		(property "Reference" "H4"
			(at 0 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "75ad2039-b9ce-421d-b2d6-afa14cceeff1")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "PastPrinterHole"
			(at 0 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "c9ae38c0-4c38-4c6a-80b8-2abbc3b92767")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "92cc2413-8434-4c69-b890-4aaae41e1520")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Past Printer Hole"
			(at 0 7.62 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca461c9a-99e6-4c5b-8a82-3e3e9298af5a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e21ab11-2673-427f-a296-0285b6712058")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "898e853a-a94b-4c19-b931-de44e8c9b6fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc861490-ce87-4497-ab1c-b89da6b75099")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed815e8c-d37c-4d5a-b150-9978dde5987e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80fa77bf-b1e0-4328-b6f3-c23780fbefcb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "70c6c446-ea97-434c-bb88-8e0b98c6c2b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/677b4100-1095-4bc0-9deb-8babf712862e")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "bb3d58e9-4e52-4b20-90ee-030d76e266db")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "033b161b-78dc-40a5-b787-a44bd850f7f7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "1b7b9ba8-0e4f-4d4a-b25c-e3a2c2f79dc1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(uuid "af681ea8-2472-43a5-bdc4-bd350fbf7eaf")
		)
		(embedded_fonts no)
	)
	(footprint "myWürthSHFU:WP-SHFU_7461098_HAL"
		(locked yes)
		(layer "F.Cu")
		(uuid "9e41e515-f8c0-4d0c-a299-48418aab0b8e")
		(at 142 165)
		(descr "WP-SHFU External thread, full plain\nDrill hole specification for HAL\nThread M6 , 25pins\nMax Height = 15.5mm")
		(property "Reference" "J4"
			(at 0 -7.6 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "513c783c-5297-43a2-ba18-f03f506045f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify bottom)
			)
		)
		(property "Value" "Würth RedCube"
			(at -3.5 8.8 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "506e1b97-e4d9-4f54-b0ee-78fd26de9da8")
			(effects
				(font
					(size 1.1684 1.1684)
					(thickness 0.1016)
				)
				(justify left bottom)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6ccabf11-2126-4376-848a-231a20884638")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M6 PRESS FIT 250A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4417a627-3024-4b4e-9ddc-c76748382b11")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "CON521"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15eb1017-b940-4be2-9a96-f9ee770811fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "7461098"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "79988b76-a5c4-484e-8b45-f84a9a87370e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3e82340-2cb3-42ad-93c7-5626dd9c2e14")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "17e07f4b-f47f-48a6-b841-18e82140f3a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "Würth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2779a054-51a1-4f4b-9daa-ac79540ea394")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c692579-676c-43f4-8110-6dda6cb1cda2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e520d8e-7b22-4f1a-86f7-2a5b04da78fa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dbea706e-ba0d-457e-8391-3dfb932772c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/a32336a8-a9c9-4273-9552-3fc0cd844afd")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -6.6 -6.6)
			(end 6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "336c738a-84b7-4f53-88a7-98db30fc6f3b")
		)
		(fp_line
			(start -6.6 6.6)
			(end -6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35fc2298-503f-4347-8a7d-1099e3b32611")
		)
		(fp_line
			(start 6.6 -6.6)
			(end 6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99e096bd-36a8-4894-86ef-2bb94715cd75")
		)
		(fp_line
			(start 6.6 6.6)
			(end -6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ecfb7356-1b5f-43f5-a757-3607e8f0ba6d")
		)
		(fp_poly
			(pts
				(xy 6.85 6.85) (xy -6.85 6.85) (xy -6.85 -6.85) (xy 6.85 -6.85)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.CrtYd")
			(uuid "a152ac6c-a06f-4c51-88e8-2bc101c92005")
		)
		(fp_line
			(start -6.5 -6.5)
			(end 6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "194726ab-e192-444a-bc9c-635ed17c30e7")
		)
		(fp_line
			(start -6.5 6.5)
			(end -6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6503c218-7e8c-4ed3-8bd8-65fbc6da0a1d")
		)
		(fp_line
			(start 6.5 -6.5)
			(end 6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1aa470d0-9b5a-4a5d-b923-b5830fa56f24")
		)
		(fp_line
			(start 6.5 6.5)
			(end -6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7aa4d942-15a2-42ed-afcb-9c176ef24776")
		)
		(pad "1" thru_hole circle
			(at -5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "0e2d3840-1499-476e-a3fa-56dcf6e06c7a")
		)
		(pad "1" thru_hole circle
			(at -5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "afc7f2f5-746f-4970-914b-3293e666543c")
		)
		(pad "1" thru_hole circle
			(at -5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "43ad4dab-4907-4c3b-be16-e38a7304d453")
		)
		(pad "1" thru_hole circle
			(at -5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "f1b0b6dd-9782-4157-8a33-5a42236f8432")
		)
		(pad "1" thru_hole circle
			(at -5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b0cbe57a-9309-4423-a0ef-daa4318da31e")
		)
		(pad "1" thru_hole circle
			(at -2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "9d143c1b-8071-4508-a8e2-950dbd865aab")
		)
		(pad "1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ef2c631b-7411-4bcf-b2f6-8c19f6dbbc3a")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ed163aea-c14c-421a-8178-c5bd697472d1")
		)
		(pad "1" thru_hole circle
			(at -2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "830dcb10-2eaa-439f-ba64-49556daacd71")
		)
		(pad "1" thru_hole circle
			(at -2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ae9bd6a6-77a4-4b88-8ab3-522b990e2628")
		)
		(pad "1" thru_hole circle
			(at 0 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "eaa34e7d-d701-4ac5-8c41-fb7af59fa0d9")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "02333063-67b2-4a2f-a06f-9df123161949")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "687b7099-0cb1-47d2-bd08-3d5684047a40")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "9cc6442d-293c-47ab-9861-735f72ca9e9a")
		)
		(pad "1" thru_hole circle
			(at 0 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "1510a0d9-ae9f-479a-b424-5c1bc845f180")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "0b56be17-b5e1-41c7-b572-cbc57f99a5f9")
		)
		(pad "1" thru_hole circle
			(at 2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "925a65e5-365b-414a-9dfb-0367453a30a4")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "67beb654-df58-40fd-84a6-e30752ef2f08")
		)
		(pad "1" thru_hole circle
			(at 2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "a51e384a-e209-4e04-92ea-b77b0f743c17")
		)
		(pad "1" thru_hole circle
			(at 2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ec85bdb5-aa47-4097-988d-9b4208ae1106")
		)
		(pad "1" thru_hole circle
			(at 5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "e883282d-7ac0-4d3b-b8d3-0bdd0f24edfe")
		)
		(pad "1" thru_hole circle
			(at 5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "c7a8662e-11f8-4936-bfa1-746307998898")
		)
		(pad "1" thru_hole circle
			(at 5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "9e2eab15-0765-42e7-a0b6-f5722b8a31e6")
		)
		(pad "1" thru_hole circle
			(at 5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "3c421817-7cc5-48e5-95f8-55854520d390")
		)
		(pad "1" thru_hole circle
			(at 5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/B+Terminal")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b3ab873d-aed8-4653-aa72-10dc2fa1e2da")
		)
		(embedded_fonts no)
		(model "D:/projekte/Kicad/8.0/3dmodels/würth_shfu_redcube_einpressbolzen/7461098.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "myHoles:printer_mounting_holes_1mm"
		(layer "F.Cu")
		(uuid "a6560c31-568b-4aab-90e6-e5dd3c909079")
		(at 235.5 295)
		(property "Reference" "H8"
			(at 0 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "1895544f-72f5-4ec1-bc51-014cd7a59919")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "PastPrinterHole"
			(at 0 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "dfb573bd-c790-4224-be6d-62394e7273f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "abae1f12-c49f-46f7-a49d-5059733d47b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Past Printer Hole"
			(at 0 7.62 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6459833e-1e87-4a1d-84b0-fb13aebc431d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d988c439-63b6-477f-b59f-9b41a384f708")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "af076fb0-8d37-4309-a39b-690520c78ecb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "075d221e-3efe-4fa3-a869-2a95b6835d11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f7f188d7-ccd3-42bd-a6d5-cb0049de2111")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3a904cf8-b52a-40bd-99ba-de8f9f3ee6c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "72267fdf-4af5-4412-a94e-3257fc309a85")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/407be68d-44df-4e73-bb0f-f94cf70703ea")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "4c1292cc-0862-46a3-b97f-71ee37b181fc")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "9bd88ff0-1bed-4db2-aee4-23572dc8ce22")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "29b87d7c-b79a-4af1-91e5-f3405937f157")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(uuid "029e66dd-adbe-4254-b37c-452cd0f03b46")
		)
		(embedded_fonts no)
	)
	(footprint "myHoles:printer_mounting_holes_1mm"
		(layer "F.Cu")
		(uuid "aea6b7cb-61b2-4cf8-832e-33028b9ad0f8")
		(at 235.5 125)
		(property "Reference" "H6"
			(at 0 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "115927a0-e82f-4902-83a9-08f971a0f76d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Value" "PastPrinterHole"
			(at 0 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "0ff68478-2ee6-45b4-8077-5033ea3a0e37")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c7ad3a92-7a6c-44c6-b295-009527f445c3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Past Printer Hole"
			(at 0 7.62 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4dc01814-bba2-4641-b2d3-f961d14296fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c70846c2-74f7-4614-9b86-58c07d4df601")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a86cb2c1-13e6-4996-851b-17edbf443bdf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1c7e5515-474e-4416-987d-730443002021")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3531fe48-5a7d-4cd6-a138-d2203d2bd77f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "751e9af1-9a41-48e1-bdb4-fb359f9ef020")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ead1ca96-9936-4c30-bdcb-18ea2530ebf4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/593929fd-aa92-4780-8250-cdd745c73e4e")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.1)
				(type default)
			)
			(fill no)
			(layer "F.SilkS")
			(uuid "867c0053-dc4b-473d-8ef4-cbc698ec62e2")
		)
		(fp_circle
			(center 0 0)
			(end 1 0)
			(stroke
				(width 0.05)
				(type default)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "17b2e9d9-5bb6-4e2a-89ee-df626a1a3c1e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "4db4dfd3-1c83-4eaf-bcdc-f4233dd25748")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(uuid "4f3cb9a0-a30c-4aa7-861c-d3c9ed0fa2b6")
		)
		(embedded_fonts no)
	)
	(footprint "myWürthSHFU:WP-SHFU_7461098_HAL_gewinkelt"
		(layer "F.Cu")
		(uuid "c6f8f7da-1d4d-486f-b17b-7d429373c81e")
		(at 204 129.25)
		(descr "WP-SHFU External thread, full plain\nDrill hole specification for HAL\nThread M6 , 25pins\nMax Height = 15.5mm")
		(property "Reference" "J2"
			(at 0 -7.6 0)
			(unlocked yes)
			(layer "F.SilkS")
			(uuid "f4e0a1fa-3020-477f-a49a-dd8c83cb9d61")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
				(justify bottom)
			)
		)
		(property "Value" "Würth RedCube"
			(at -3.5 8.8 0)
			(unlocked yes)
			(layer "F.Fab")
			(uuid "eb3b4c2f-a09c-4d21-88b7-83facc3f4464")
			(effects
				(font
					(size 1.1684 1.1684)
					(thickness 0.1016)
				)
				(justify left bottom)
			)
		)
		(property "Datasheet" "https://www.we-online.com/de/components/products/REDCUBE_PRESS-FIT_RIGHT_ANGLED_EDGE_POSITION"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a09d7ade-a7d1-4b07-a117-5583d7b3c075")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M6 PRESS FIT 250A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f68c6793-8c64-4a6d-8572-b271a654dd70")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "CON529"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "15b1e31d-3a90-4609-9753-9897626d6e3b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "74622106"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "01c4d419-7dda-424b-a2d5-da7c733eabec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4c59afe-bcc2-447a-b3d8-e85bc6906606")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6e893e84-87a5-4406-93a0-e97f58c5f114")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "Würth"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1de25541-74a5-4215-a05f-457faf5ef31f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f15e81f5-48cd-42a0-9109-17914667c1d5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "286ab33b-57d0-4970-9ec5-abaf00c050e7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7ac9ab6c-43b7-47ea-9312-462cfb620677")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/7dd09515-a35f-463b-bd8d-d919fb13dadd")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -6.6 -6.6)
			(end 6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba009929-50b1-4d77-b794-c890950a08cb")
		)
		(fp_line
			(start -6.6 6.6)
			(end -6.6 -6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee38b98b-69de-4f85-ad38-939ec78875c9")
		)
		(fp_line
			(start -6.5 -9.25)
			(end -6.5 3.75)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "9573e767-5828-4bac-843f-d3f9f6df2c5b")
		)
		(fp_line
			(start -6.5 3.75)
			(end 6.5 3.75)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "587a9ed6-b3d7-4143-88b7-2447a47fedac")
		)
		(fp_line
			(start 6.5 -9.25)
			(end -6.5 -9.25)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "7a38ccf9-8fbc-4911-bf4a-cd9bba1ec061")
		)
		(fp_line
			(start 6.5 3.75)
			(end 6.5 -9.25)
			(stroke
				(width 0.2)
				(type dash)
			)
			(layer "F.SilkS")
			(uuid "6057458f-fd09-48ef-a902-34df0d643a9a")
		)
		(fp_line
			(start 6.6 -6.6)
			(end 6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9dd4293d-6b8b-48cb-acb5-c9a05d5a18df")
		)
		(fp_line
			(start 6.6 6.6)
			(end -6.6 6.6)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "357720e0-f299-459a-a171-f755e5a7671d")
		)
		(fp_poly
			(pts
				(xy 6.85 6.85) (xy -6.85 6.85) (xy -6.85 -6.85) (xy 6.85 -6.85)
			)
			(stroke
				(width 0)
				(type default)
			)
			(fill yes)
			(layer "F.CrtYd")
			(uuid "9bc42ddd-11b9-400d-b2aa-cb033c4b9a19")
		)
		(fp_line
			(start -6.5 -6.5)
			(end 6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8465b2a0-cd1c-4798-a57f-e37ccd007318")
		)
		(fp_line
			(start -6.5 6.5)
			(end -6.5 -6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94dd1715-a8a7-433d-8d66-7aa01efb4361")
		)
		(fp_line
			(start 6.5 -6.5)
			(end 6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b48ed456-165c-4be9-a15c-71c6cb82b9ea")
		)
		(fp_line
			(start 6.5 6.5)
			(end -6.5 6.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cee306f-dcdd-412c-9c47-8afbd1e36f9c")
		)
		(pad "1" thru_hole circle
			(at -5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "715a16b5-1cf1-4684-9363-0773e5fc106c")
		)
		(pad "1" thru_hole circle
			(at -5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b198645d-fe62-420b-bdfa-63e7a13578f5")
		)
		(pad "1" thru_hole circle
			(at -5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ed64ebf1-2d29-4b76-a935-b64ee3ce1241")
		)
		(pad "1" thru_hole circle
			(at -5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "3fcaca0a-dff1-4af1-9aac-1c73def955ca")
		)
		(pad "1" thru_hole circle
			(at -5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "50a73491-d4eb-4134-a15b-494673b611d3")
		)
		(pad "1" thru_hole circle
			(at -2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "040987b8-ca53-4c43-b259-2498a5e03059")
		)
		(pad "1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "653c6fd4-5eac-4db9-a660-162c5157a4d9")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "d055895d-7193-4163-b6b0-c9857d11f40a")
		)
		(pad "1" thru_hole circle
			(at -2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "0530d85d-484c-4c41-857f-02048f2972d8")
		)
		(pad "1" thru_hole circle
			(at -2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "de4630b6-1437-4203-8e9c-c75a487064df")
		)
		(pad "1" thru_hole circle
			(at 0 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ad5ec4a2-afc0-4ff7-a948-133257c4fcfc")
		)
		(pad "1" thru_hole circle
			(at 0 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "84b72d73-5c8f-4b78-8a3c-54dcd8c5ffe3")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "f79eb5da-a0fb-453f-ad48-e7a78fe7df5b")
		)
		(pad "1" thru_hole circle
			(at 0 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "18a528c8-c03d-4bc7-8381-7ce3f48d9fea")
		)
		(pad "1" thru_hole circle
			(at 0 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "f7e94eee-c396-41d7-8a81-da68d1b94198")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "ab45a5f4-5447-4ca9-b000-3d6e4315b27c")
		)
		(pad "1" thru_hole circle
			(at 2.54 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "dbe2a66d-4d87-4374-8154-aee7783cc588")
		)
		(pad "1" thru_hole circle
			(at 2.54 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "328e89ed-69a5-4e56-bc1d-76be3a788d1b")
		)
		(pad "1" thru_hole circle
			(at 2.54 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "568d4a23-b608-4912-8cac-9b8c0ac2174b")
		)
		(pad "1" thru_hole circle
			(at 2.54 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "d4ebdfc4-a9d4-434f-8825-1841254780e1")
		)
		(pad "1" thru_hole circle
			(at 5.08 -5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "1786629b-a6a2-4f12-97b1-7fd810e7ba11")
		)
		(pad "1" thru_hole circle
			(at 5.08 -2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "23296641-f92d-4f2c-8dc7-85d007c382cd")
		)
		(pad "1" thru_hole circle
			(at 5.08 0)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "b9d4fc8b-5eeb-4be7-a354-2e9a06928c84")
		)
		(pad "1" thru_hole circle
			(at 5.08 2.54)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "3a167b72-7590-4c7e-b1aa-b61bc49732fc")
		)
		(pad "1" thru_hole circle
			(at 5.08 5.08)
			(size 2.2 1.8)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
			(uuid "64d7fd38-9e46-4210-8378-cd296e507699")
		)
		(embedded_fonts no)
		(model "D:/projekte/Kicad/8.0/3dmodels/würth_shfu_redcube_einpressbolzen/74622106.stp"
			(offset
				(xyz 0 2.54 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad"
		(layer "F.Cu")
		(uuid "c87311b8-42f8-499f-8e5b-e4e79ed2382d")
		(at 103 295)
		(descr "Mounting Hole 2.2mm, M2, DIN965")
		(tags "mounting hole 2.2mm m2 din965")
		(property "Reference" "H1"
			(at 0 -2.9 0)
			(layer "F.SilkS")
			(uuid "2a8c3ece-14f6-4fe3-a14b-3b6b26e3879b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 2.9 0)
			(layer "F.Fab")
			(uuid "deb84df5-b922-4b01-b0cf-fd20d64d3550")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "69501609-ee7c-4616-8cb5-bc593399ea7d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "08d39a70-8bdc-4508-b388-a2e56fd462df")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "793ad5c9-4369-4f28-be75-f8e9510aa7f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d2076169-9be1-4d55-b072-f860a82784aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fef87c55-8aef-4918-aee1-43fde384f09c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "56cb987a-c6fb-42a1-9353-680d093ac6a8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6ae3599-1c4f-4688-b46e-ce869a18ea2d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "afa689a0-a2a4-4d9e-8de7-4f49dc7dbaa8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(path "/7739b16e-fba9-43c9-af73-46dfcb628882")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.9 0)
			(stroke
				(width 0.15)
				(type solid)
			)
			(fill no)
			(layer "Cmts.User")
			(uuid "df26788a-d5de-4066-93c1-49c7de010385")
		)
		(fp_circle
			(center 0 0)
			(end 2.15 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ab733a11-ef2f-4a30-9ecd-4ad136ffd72a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c7367338-0ed9-48c2-bbbe-6d4f92aabdf1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.8 3.8)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(H1-Pad1)")
			(pinfunction "1")
			(pintype "input+no_connect")
			(uuid "d6557e87-6cb7-40fa-acc4-d42a94443843")
		)
		(embedded_fonts no)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "F.Cu")
		(uuid "d15982f0-ef78-45c0-8ef4-398ccdbaa5cc")
		(at 118 295)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID1"
			(at 0 -2.54 0)
			(layer "F.SilkS")
			(uuid "c1dc10de-21c7-4475-b715-1f4768e8b97b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fiducial"
			(at 0 2.286 0)
			(layer "F.Fab")
			(uuid "5d0edcb0-d612-4d1f-afe4-c2f90c26e3b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "22a58ec0-b077-4137-a0af-9d3c4d1de622")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c65b0ef7-928a-4bac-aa4e-df805728e4ae")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a553bc1-6261-4f5a-9eb8-68817c77af7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0f3441be-352c-4b72-99ac-d837e07d0ddd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "902ee695-6bfc-4080-be3e-a5cace70e588")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4919839-3503-4eb4-968e-554eadeb6069")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06af586b-cfe5-4eca-8bc7-248e6411fd5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a69377e5-e631-482e-a849-7a6fce5e8d5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "679a8cd2-17ad-46fd-bab9-61356891e3f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e31cda2a-0346-4659-8196-dc1cc1bd5af6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/5f9e64aa-3d81-4b2b-bd1d-113459de8c53")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a0851adb-95ed-48e7-9cb8-ccce71b191c3")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "38edd87e-bf69-4231-89b7-91b182984d8d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a55fd89a-f257-41f6-b0bb-c1c6716c381e")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "703bf79e-4af7-4eb3-a2b1-4e26740df102")
		)
		(embedded_fonts no)
	)
	(footprint "Fiducial:Fiducial_1mm_Mask3mm"
		(layer "F.Cu")
		(uuid "f254f4b9-641d-4e97-bd96-7560d262024e")
		(at 115.5 125)
		(descr "Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)")
		(tags "fiducial")
		(property "Reference" "FID2"
			(at 0 -2.54 0)
			(layer "F.SilkS")
			(uuid "2f334899-b899-4840-9b83-ec679f05e969")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Fiducial"
			(at 0 2.286 0)
			(layer "F.Fab")
			(uuid "3a1e1be0-2678-4c99-bf80-db6f50bef2b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a1b8950a-540e-4aa4-9807-fa9d14049f6a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Fiducial Marker"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2beb7325-f970-407e-ba07-4976071c53ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "ECS Art#" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d22ac928-3a69-4de1-9daf-cba7911c7beb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "HAN" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f94e3118-e758-4640-b178-06c04509ea85")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Voltage" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "87968740-5391-4f92-b6aa-b8876986b139")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Toleranz" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5a1a98a1-da9e-4816-8a7e-5b206893b149")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Hersteller" "---"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "831da04b-df89-4f1f-823d-8b8245e8a6db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Field-1" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d41dafe8-5d52-4382-95df-185b7bb89dc9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Device" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dee747fd-b1d3-4202-9c4a-801c22f9d32f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Sim.Pins" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8545a88-7baf-41cb-9aef-4d8364533584")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Fiducial*")
		(path "/6f1cf190-689f-4d03-b5dc-05a38d2acdbe")
		(sheetname "/")
		(sheetfile "smartSwitch.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_circle
			(center 0 0)
			(end 1.75 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "4ee50561-d99b-44d1-8ea5-7ec4fd56cd01")
		)
		(fp_circle
			(center 0 0)
			(end 1.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "054a2c55-50ed-456c-b224-0dfcd5b3241d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5bf23512-eae4-439a-99e1-ba8cc9132cbf")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 1)
			(clearance 1)
			(uuid "74c35bcf-c66a-4cb3-b9ea-c5ef2752dc13")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 232 130)
		(end 237 130)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "0fa37eb9-82ef-4303-8cb2-7654808e5da0")
	)
	(gr_arc
		(start 239 168)
		(mid 238.414214 169.414214)
		(end 237 170)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "100031ec-35f3-485e-8663-1598f80aa324")
	)
	(gr_arc
		(start 116 288)
		(mid 115.414214 289.414214)
		(end 114 290)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "2438d367-f5cf-46fb-b30b-5796f88ef37d")
	)
	(gr_arc
		(start 114 130)
		(mid 115.414214 130.585786)
		(end 116 132)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "2b41154b-261c-4a6e-afee-139dba8f541b")
	)
	(gr_line
		(start 237 170)
		(end 232 170)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "2c2fffcd-50a2-49dc-98be-bb6f82954916")
	)
	(gr_arc
		(start 116 168)
		(mid 115.414214 169.414214)
		(end 114 170)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "3461b7c0-00cd-45b8-998e-24c15fe55ef9")
	)
	(gr_line
		(start 232 250)
		(end 237 250)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "49eaf55a-096a-4d14-85c1-0bebe916f6ce")
	)
	(gr_line
		(start 230 168)
		(end 230 132)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "4a78af82-1ebb-4f33-b693-ebe55596893c")
	)
	(gr_arc
		(start 107 132)
		(mid 107.585786 130.585786)
		(end 109 130)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "54ce4c6b-d00a-493b-8805-8d5be26478bc")
	)
	(gr_arc
		(start 237 250)
		(mid 238.414214 250.585786)
		(end 239 252)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "56cce633-dcdc-4d00-ab72-1f35b01bfa11")
	)
	(gr_line
		(start 107 288)
		(end 107 252)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "5fbb3fb0-c270-4262-b9a1-8399a11a8a27")
	)
	(gr_line
		(start 116 132)
		(end 116 168)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "600a3631-f8c0-42a6-989b-9925586fb9cc")
	)
	(gr_line
		(start 109 250)
		(end 114 250)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "619a8f5b-fdd9-47a2-90b0-830d80038430")
	)
	(gr_arc
		(start 237 130)
		(mid 238.414214 130.585786)
		(end 239 132)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6251c4dc-94c7-458a-abfb-058622a3f4df")
	)
	(gr_rect
		(start 100 120)
		(end 246 300)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "6cff1f51-cd01-47e1-a2b7-98a2ee291ff2")
	)
	(gr_arc
		(start 114 250)
		(mid 115.414214 250.585786)
		(end 116 252)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6f4cfd1a-5777-4d7c-acf3-3b653a5b6cd7")
	)
	(gr_arc
		(start 239 288)
		(mid 238.414214 289.414214)
		(end 237 290)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "6fb37e1c-09bf-447f-a021-222f4cd0a790")
	)
	(gr_line
		(start 107 168)
		(end 107 132)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "8511792e-9f6a-4292-a40b-e4f91c45f37d")
	)
	(gr_line
		(start 114 290)
		(end 109 290)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "8c998fd8-378a-481e-81fb-b12d0a1bcae8")
	)
	(gr_line
		(start 109 130)
		(end 114 130)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "8d88ecb1-4bc9-4303-90b3-10a5a3b618e5")
	)
	(gr_line
		(start 237 290)
		(end 232 290)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "945185e4-f3f1-4bb5-819a-b527390b65d4")
	)
	(gr_arc
		(start 109 170)
		(mid 107.585786 169.414214)
		(end 107 168)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "9dadf85b-66e5-43eb-bfc3-5fd7168ebbbb")
	)
	(gr_arc
		(start 232 170)
		(mid 230.585786 169.414214)
		(end 230 168)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "b3459237-a43a-4b7b-96fc-73ac7f31cd10")
	)
	(gr_arc
		(start 109 290)
		(mid 107.585786 289.414214)
		(end 107 288)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "b8493d5d-e81d-4bc7-a924-4af2981193b6")
	)
	(gr_arc
		(start 230 252)
		(mid 230.585786 250.585786)
		(end 232 250)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "c905720c-4364-4e8c-8f88-2a86fb023126")
	)
	(gr_line
		(start 239 252)
		(end 239 288)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "d07e315f-83dc-4a54-bf01-5352690723a5")
	)
	(gr_arc
		(start 232 290)
		(mid 230.585786 289.414214)
		(end 230 288)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "d3c41331-53f0-407a-8031-a260c5fa86c6")
	)
	(gr_line
		(start 239 132)
		(end 239 168)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "e240fee1-7140-4fd6-ab03-47617814feee")
	)
	(gr_arc
		(start 230 132)
		(mid 230.585786 130.585786)
		(end 232 130)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "e6a58662-a31f-467e-b40b-c7ab4239b022")
	)
	(gr_line
		(start 116 252)
		(end 116 288)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "e8f1036b-c74a-471e-ae2d-a2c0f4eb05aa")
	)
	(gr_line
		(start 230 288)
		(end 230 252)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "ea033540-f8a3-492f-bf74-f2cc2cf6a90b")
	)
	(gr_arc
		(start 107 252)
		(mid 107.585786 250.585786)
		(end 109 250)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "ea541105-2274-4b6b-a50d-0eccd3236049")
	)
	(gr_line
		(start 114 170)
		(end 109 170)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "fe4fe82d-3eac-457c-9c0d-5d86f03214a3")
	)
	(gr_rect
		(start 225 245)
		(end 244 295)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "3263bc68-6950-476f-968d-8baedcde5e5f")
	)
	(gr_rect
		(start 225 125)
		(end 244 175)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "5e3acf6b-cd41-4843-9e7f-b675fe40acfa")
	)
	(gr_rect
		(start 102 125)
		(end 121 175)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "63271691-5aad-4a18-9be0-218b27c7a8c8")
	)
	(gr_rect
		(start 102 245)
		(end 121 295)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "ec4c5c54-c4db-46c2-a7a6-013987699c52")
	)
	(gr_line
		(start 173 120)
		(end 173 300)
		(stroke
			(width 0.1)
			(type dash_dot)
		)
		(layer "User.2")
		(uuid "13af49cf-d4ca-4d8f-a8d5-36a14d506e69")
	)
	(gr_line
		(start 273 210)
		(end 73 210)
		(stroke
			(width 0.1)
			(type dash_dot)
		)
		(layer "User.2")
		(uuid "73f93f8e-63ec-4b49-8aee-3e139315c46c")
	)
	(gr_line
		(start 123 257.5)
		(end 123.25 257.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.3")
		(uuid "73a2ad5e-b273-4787-8672-b8f579d2ebe5")
	)
	(gr_line
		(start 123.25 150)
		(end 123 150)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "User.3")
		(uuid "90eaadb6-fe2d-44d9-afa6-07f4a5d7d444")
	)
	(gr_text_box "Abstand AB1: 50mm\nAbstand Relais: 65mm \nAbstzand Shunt 60mm (17,65 SENSE Pins)\n"
		(start 49.95 39.75)
		(end 83.55 59.55)
		(margins 0.8 0.8 0.8 0.8)
		(layer "User.1")
		(uuid "0d5e6914-d3e0-4c2c-ad80-ffa0bbad64f7")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left top)
		)
		(border yes)
		(stroke
			(width 0.1)
			(type solid)
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(uuid "01c236e6-8380-426b-9848-82161b5eef7e")
		(pts
			(xy 246 120) (xy 100 120)
		)
		(height 20)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "146,0000 mm"
			(at 173 98.85 0)
			(layer "User.2")
			(uuid "01c236e6-8380-426b-9848-82161b5eef7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(uuid "182b8976-150b-4078-a8fb-c54755abd034")
		(pts
			(xy 252 210) (xy 252 120)
		)
		(height 6)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "90,0000 mm"
			(at 256.85 165 90)
			(layer "User.2")
			(uuid "182b8976-150b-4078-a8fb-c54755abd034")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(uuid "37312c86-25dc-4c64-9686-e422ec31cf2a")
		(pts
			(xy 246 120) (xy 173 120)
		)
		(height 17.5)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "73,0000 mm"
			(at 209.5 101.35 0)
			(layer "User.2")
			(uuid "37312c86-25dc-4c64-9686-e422ec31cf2a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(uuid "4781d56c-8161-48c3-9307-4d586e2aa7f5")
		(pts
			(xy 254.5 120) (xy 254.5 300)
		)
		(height -8.5)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "180,0000 mm"
			(at 265.639649 210.889649 90)
			(layer "User.2")
			(uuid "4781d56c-8161-48c3-9307-4d586e2aa7f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(uuid "7e9090fa-f897-41ce-9227-26fdb3110e99")
		(pts
			(xy 173 120) (xy 100 120)
		)
		(height 17.5)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "73,0000 mm"
			(at 136.5 101.35 0)
			(layer "User.2")
			(uuid "7e9090fa-f897-41ce-9227-26fdb3110e99")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(uuid "c2038cc5-f606-4d91-b402-0de152e541ec")
		(pts
			(xy 173 120) (xy 204 120)
		)
		(height -4.75)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "31,0000 mm"
			(at 188.5 114.1 0)
			(layer "User.2")
			(uuid "c2038cc5-f606-4d91-b402-0de152e541ec")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type aligned)
		(layer "User.2")
		(uuid "daa8074b-dd64-4b10-b130-3a162b75c503")
		(pts
			(xy 252 300) (xy 252 210)
		)
		(height 6)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "90,0000 mm"
			(at 256.85 255 90)
			(layer "User.2")
			(uuid "daa8074b-dd64-4b10-b130-3a162b75c503")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "03ada09a-f167-43db-a2ab-6e788d205fd6")
		(pts
			(xy 114 132) (xy 100 120)
		)
		(height -19.5)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "14,0000 mm"
			(at 107 111.35 0)
			(layer "User.2")
			(uuid "03ada09a-f167-43db-a2ab-6e788d205fd6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "1198e10e-0f1b-44cc-a8e2-705d75ba0382")
		(pts
			(xy 109 288) (xy 100 300)
		)
		(height 17)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "9,0000 mm"
			(at 104.5 303.85 0)
			(layer "User.2")
			(uuid "1198e10e-0f1b-44cc-a8e2-705d75ba0382")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "2ea86baf-f8d5-4ee7-be49-2199aafa3128")
		(pts
			(xy 114 132) (xy 114 168)
		)
		(height -18.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "36,0000 mm"
			(at 94.35 150 90)
			(layer "User.2")
			(uuid "2ea86baf-f8d5-4ee7-be49-2199aafa3128")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "2f3ff9dc-10ea-4160-9313-d90c4b502abe")
		(pts
			(xy 232 132) (xy 246 132)
		)
		(height -22)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "14,0000 mm"
			(at 239 108.85 0)
			(layer "User.2")
			(uuid "2f3ff9dc-10ea-4160-9313-d90c4b502abe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "31f27f77-9114-488a-86ef-1181b059e010")
		(pts
			(xy 237 288) (xy 246 300)
		)
		(height 16)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "12,0000 mm"
			(at 251.85 294 90)
			(layer "User.2")
			(uuid "31f27f77-9114-488a-86ef-1181b059e010")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "39296c2d-c2a1-45dc-8fe1-4e1da0125249")
		(pts
			(xy 114 288) (xy 114 252)
		)
		(height -18.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "36,0000 mm"
			(at 94.35 270 90)
			(layer "User.2")
			(uuid "39296c2d-c2a1-45dc-8fe1-4e1da0125249")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "4ddfd0a2-5bd0-41c7-a6e1-7fc35b196fe3")
		(pts
			(xy 142 128.5) (xy 173 128)
		)
		(height -13.25)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "31,0000 mm"
			(at 157.5 114.1 0)
			(layer "User.2")
			(uuid "4ddfd0a2-5bd0-41c7-a6e1-7fc35b196fe3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "6a1d4f0c-15f0-4d45-8200-d60f7b45aec9")
		(pts
			(xy 109 288) (xy 109.25 300)
		)
		(height -13.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "12,0000 mm"
			(at 94.35 294 90)
			(layer "User.2")
			(uuid "6a1d4f0c-15f0-4d45-8200-d60f7b45aec9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "8a88a3d6-1266-470c-920e-84201aab4f68")
		(pts
			(xy 232 288) (xy 232 252)
		)
		(height 21)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "36,0000 mm"
			(at 251.85 270 90)
			(layer "User.2")
			(uuid "8a88a3d6-1266-470c-920e-84201aab4f68")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "93bd038b-0664-4b4f-8709-6fef211f7f7e")
		(pts
			(xy 237 132) (xy 246 132.25)
		)
		(height -17)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "9,0000 mm"
			(at 241.5 113.85 0)
			(layer "User.2")
			(uuid "93bd038b-0664-4b4f-8709-6fef211f7f7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "a6c1742b-9f18-4ca3-ad2e-9356dcd3bf0a")
		(pts
			(xy 237 132) (xy 237 168)
		)
		(height 13.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "36,0000 mm"
			(at 249.35 150 90)
			(layer "User.2")
			(uuid "a6c1742b-9f18-4ca3-ad2e-9356dcd3bf0a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "c0c220a7-028c-4d2d-8c70-28d9b02c0e7d")
		(pts
			(xy 237 132) (xy 237.5 120)
		)
		(height 13.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "12,0000 mm"
			(at 249.35 126 90)
			(layer "User.2")
			(uuid "c0c220a7-028c-4d2d-8c70-28d9b02c0e7d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "c75b3947-17f8-4c00-af51-2fde72632e3e")
		(pts
			(xy 100 120) (xy 100 132)
		)
		(height -4.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "12,0000 mm"
			(at 94.35 126 90)
			(layer "User.2")
			(uuid "c75b3947-17f8-4c00-af51-2fde72632e3e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "cb13010e-3482-4b0d-aa88-8bf9fe2776cb")
		(pts
			(xy 232 288) (xy 246 300)
		)
		(height 19.5)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "14,0000 mm"
			(at 239 306.35 0)
			(layer "User.2")
			(uuid "cb13010e-3482-4b0d-aa88-8bf9fe2776cb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "d5c668e9-28fd-40c5-b367-ac4f6d6f3316")
		(pts
			(xy 109 132) (xy 100 120)
		)
		(height -14.5)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "9,0000 mm"
			(at 104.5 116.35 0)
			(layer "User.2")
			(uuid "d5c668e9-28fd-40c5-b367-ac4f6d6f3316")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.2")
		(uuid "ff3d0011-6d4c-45f2-b7cb-98bf70387919")
		(pts
			(xy 114 288) (xy 100 300)
		)
		(height 22)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "14,0000 mm"
			(at 107 308.85 0)
			(layer "User.2")
			(uuid "ff3d0011-6d4c-45f2-b7cb-98bf70387919")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
	)
	(group ""
		(uuid "1a193fff-6a53-4fbd-8fa3-5b8d2f02ebb4")
		(members "49eaf55a-096a-4d14-85c1-0bebe916f6ce" "56cce633-dcdc-4d00-ab72-1f35b01bfa11"
			"6fb37e1c-09bf-447f-a021-222f4cd0a790" "945185e4-f3f1-4bb5-819a-b527390b65d4"
			"c905720c-4364-4e8c-8f88-2a86fb023126" "d07e315f-83dc-4a54-bf01-5352690723a5"
			"d3c41331-53f0-407a-8031-a260c5fa86c6" "ea033540-f8a3-492f-bf74-f2cc2cf6a90b"
		)
	)
	(group ""
		(uuid "29264d2e-7bbe-4b56-9cd8-bdfb232daf11")
		(members "2438d367-f5cf-46fb-b30b-5796f88ef37d" "5fbb3fb0-c270-4262-b9a1-8399a11a8a27"
			"619a8f5b-fdd9-47a2-90b0-830d80038430" "6f4cfd1a-5777-4d7c-acf3-3b653a5b6cd7"
			"8c998fd8-378a-481e-81fb-b12d0a1bcae8" "b8493d5d-e81d-4bc7-a924-4af2981193b6"
			"e8f1036b-c74a-471e-ae2d-a2c0f4eb05aa" "ea541105-2274-4b6b-a50d-0eccd3236049"
		)
	)
	(group ""
		(uuid "4d9c1712-46c0-4529-8e5e-ba2e006cec25")
		(members "2b41154b-261c-4a6e-afee-139dba8f541b" "3461b7c0-00cd-45b8-998e-24c15fe55ef9"
			"54ce4c6b-d00a-493b-8805-8d5be26478bc" "600a3631-f8c0-42a6-989b-9925586fb9cc"
			"8511792e-9f6a-4292-a40b-e4f91c45f37d" "8d88ecb1-4bc9-4303-90b3-10a5a3b618e5"
			"9dadf85b-66e5-43eb-bfc3-5fd7168ebbbb" "fe4fe82d-3eac-457c-9c0d-5d86f03214a3"
		)
	)
	(group ""
		(uuid "f708e5b3-6fdf-4def-9900-c60938296a78")
		(members "0fa37eb9-82ef-4303-8cb2-7654808e5da0" "100031ec-35f3-485e-8663-1598f80aa324"
			"2c2fffcd-50a2-49dc-98be-bb6f82954916" "4a78af82-1ebb-4f33-b693-ebe55596893c"
			"6251c4dc-94c7-458a-abfb-058622a3f4df" "b3459237-a43a-4b7b-96fc-73ac7f31cd10"
			"e240fee1-7140-4fd6-ab03-47617814feee" "e6a58662-a31f-467e-b40b-c7ab4239b022"
		)
	)
	(embedded_fonts no)
)
