(footprint "WIRE-TO-BOARD-(REV18A)_61200621721"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "WR-BHD 2.54mm Male Angled Box Header, 6 Pins")
	(property "Reference" "REF**"
		(at 8.6504 4.0679 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "74ef08fa-499c-49f9-b097-ce291faa6c06")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Value" "WIRE-TO-BOARD-(REV18A)_61200621721"
		(at 8.7504 6.457 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a7c488a4-3045-4ead-b78f-2f4f104180c4")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "6ddc06f3-bef0-48db-a7a6-70764e154572")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e528cc38-7415-4f42-89a9-802b6552759b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "fe8dffea-8316-4365-83e3-e0f6100d8f84")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -7.64 3.11)
		(end 7.64 3.11)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "71424276-6fbd-4852-935c-60de143b76e5")
	)
	(fp_line
		(start -7.64 11.96)
		(end -7.64 3.11)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "90b87ed8-5c24-44e7-91ea-1abb3e43d23b")
	)
	(fp_line
		(start 7.64 3.11)
		(end 7.64 11.96)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3916476d-624a-4b61-8ab0-1d6728ac7b81")
	)
	(fp_line
		(start 7.64 11.96)
		(end -7.64 11.96)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b4a5a529-d743-4b7b-bbb6-08538ec4946e")
	)
	(fp_poly
		(pts
			(xy 7.9535 12.2735) (xy -7.9535 12.2735) (xy -7.9535 -2.3135) (xy 7.9535 -2.3135)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.CrtYd")
		(uuid "ca30fad3-3331-45c4-b6aa-dd01c34bc9c9")
	)
	(fp_text user "1"
		(at 3.905 -0.635 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5a584e6e-a989-404a-a971-decbc2026f2c")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(fp_text user "6"
		(at -4.575 2.005 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "34080ba6-7e31-41b3-b9d9-5c09b520859a")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(fp_text user "2"
		(at 3.805 2.105 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "683e3922-83f4-4190-998f-8bdebd198288")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(fp_text user "1"
		(at 3.905 -0.635 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "c16043d3-1f74-46e2-b64d-eb527229ab01")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(pad "1" thru_hole circle
		(at 2.54 -1.27)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "7b4077e7-bd90-4168-ae26-887375766198")
	)
	(pad "2" thru_hole circle
		(at 2.54 1.27)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "9677c082-c893-482b-b3d8-fe944c2e5388")
	)
	(pad "3" thru_hole circle
		(at 0 -1.27)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ac4918fa-b08f-445b-91f2-786c07843ac0")
	)
	(pad "4" thru_hole circle
		(at 0 1.27)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "c011d601-6b5f-43c4-a9f5-dd39187647ad")
	)
	(pad "5" thru_hole circle
		(at -2.54 -1.27)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bb242295-8893-4f44-9701-5d829dc48315")
	)
	(pad "6" thru_hole circle
		(at -2.54 1.27)
		(size 1.65 1.65)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "ae1f8a12-2724-4829-a25c-e710b5c24c27")
	)
)
