(footprint "SIGNALCOMMUNICATIONS-(REV18E)_WE-LQFS_48X8"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ee73fc0e-6144-42c1-a9c0-4a57c61d54a7")
		(effects
			(font
				(size 0.747776 0.747776)
				(thickness 0.065024)
			)
			(justify bottom)
		)
	)
	(property "Value" "SIGNALCOMMUNICATIONS-(REV18E)_WE-LQFS_48X8"
		(at -1.9 3.7 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ec6499d5-6fec-47f3-9af4-9601ab2db831")
		(effects
			(font
				(size 0.747776 0.747776)
				(thickness 0.065024)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "cc982f7a-dc96-4913-bb52-41e30b003e93")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "4af5c5bd-d9f2-4a99-b072-8e6d58584408")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d58644bf-8075-495c-a1c5-443ef8cf02af")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -2.4 -2.4)
		(end 2.4 -2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ba9fb2ff-adec-4f08-b258-4a13f9b20b2c")
	)
	(fp_line
		(start -2.4 -2)
		(end -2.4 -2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "095a86d6-53ff-4886-8866-6bf3f667c566")
	)
	(fp_line
		(start -2.4 2)
		(end -2.4 2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "116b0709-139c-47b5-a07a-5ffc5a88fb4e")
	)
	(fp_line
		(start 2.4 -2)
		(end 2.4 -2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "86862d83-92d1-42e4-9456-a5e48db6365f")
	)
	(fp_line
		(start 2.4 2)
		(end 2.4 2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2a4b90f2-5074-4292-9aa1-8e3f179fdd5d")
	)
	(fp_line
		(start 2.4 2.4)
		(end -2.4 2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9bb96f69-0c7f-4d36-8555-1fe5bf46364e")
	)
	(fp_poly
		(pts
			(xy 2.9635 2.7135) (xy -2.9635 2.7135) (xy -2.9635 -2.7135) (xy 2.9635 -2.7135)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.CrtYd")
		(uuid "60806fc2-3bec-45c2-ad41-ba4ad8eeb4d2")
	)
	(fp_line
		(start -2.4 -2.4)
		(end 2.4 -2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "872c7806-a8ed-4b55-b7e2-cb55e26c37bb")
	)
	(fp_line
		(start -2.4 2.4)
		(end -2.4 -2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b6a9b70c-3780-4de1-9153-00afca25e27b")
	)
	(fp_line
		(start -2.4 2.4)
		(end 2.4 2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1d68eb4d-1890-42b2-a7b8-e714ddceee1d")
	)
	(fp_line
		(start 2.4 -2.4)
		(end 2.4 2.4)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "82f49921-4806-407b-86d4-c6ad247c62c0")
	)
	(pad "1" smd rect
		(at -1.7 0 90)
		(size 3.6 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "e7ff03ed-05a9-4b94-9bf4-1e318cfacc74")
	)
	(pad "2" smd rect
		(at 1.7 0 90)
		(size 3.6 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "dcd8e691-1599-4765-acbc-472cb77f7b64")
	)
)
