(footprint "WüRTH_WIRE-TO-BOARD_61900311021"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "WR-WTB 2.54mm Right Angled Locking Header Bottom Locking, 3 Pins")
	(property "Reference" "REF**"
		(at 4.785 6.05 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a04f9031-3398-4f16-84ab-eaa9980fdf5a")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Value" "WüRTH_WIRE-TO-BOARD_61900311021"
		(at 5.01 8.03 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a1a091c4-48ed-4bbe-b930-9206770612fe")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "15f488db-833a-41c1-bd0a-92e521bbd183")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "10daddea-737a-4fee-86ff-d25fcc554422")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2c953b58-c41c-4d61-8648-88b89511a1b9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -5.23 -0.93)
		(end 2.69 -0.93)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "646d09fa-adb3-45c3-b25a-988b912288d8")
	)
	(fp_line
		(start -5.23 13.1)
		(end -5.23 -0.93)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "35cd5e73-453e-4d21-99b7-9af9710aae96")
	)
	(fp_line
		(start 2.69 -0.93)
		(end 2.69 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "58c39197-775f-4f8e-9357-9442a6f4888e")
	)
	(fp_line
		(start 2.69 13.1)
		(end -5.23 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f83f92db-575b-4a67-bc20-5be0d6ef599b")
	)
	(fp_line
		(start -5.23 0)
		(end 2.69 0)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c1654aba-5c52-4c3d-9131-baf4c65b5ccf")
	)
	(fp_line
		(start -5.23 13.1)
		(end -5.23 0)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "90b1b98b-3128-4f13-bf2c-1cfc93e36714")
	)
	(fp_line
		(start 2.69 0)
		(end 2.69 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8a64d39e-9a57-40f2-8aa8-08af0e753466")
	)
	(fp_line
		(start 2.69 13.1)
		(end -5.23 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8687958d-e75f-44cc-86ba-de93229fe42c")
	)
	(fp_text user "1"
		(at 0.635 0.635 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1856df5b-9164-4d7d-af93-009604f0f193")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(fp_text user "3"
		(at -4.445 0.635 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "37bd35ed-379f-43c5-8678-28e01cd1ae8b")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(pad "1" thru_hole circle
		(at 1.27 0)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "4a6808bd-8fa1-41a4-b129-4b71eb61f9e2")
	)
	(pad "2" thru_hole circle
		(at -1.27 0)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "6ab4e7c4-918c-4cd6-b170-a9f553404661")
	)
	(pad "3" thru_hole circle
		(at -3.81 0)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "56979cf9-e1de-4539-bb4b-c15466bc9915")
	)
)
