(footprint "TEXAS_SOIC8-POWERPAD"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "PowerPAD SOIC - 1.7 mm max height")
	(property "Reference" "REF**"
		(at -2.667 1.905 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "165e5b9f-30a6-4cd7-a191-291a4397c91a")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Value" "TEXAS_SOIC8-POWERPAD"
		(at 3.937 1.905 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "add196ef-ffa1-4590-b8ac-c0f8358866f6")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3eda7d17-dc84-486d-8667-569b8e307c27")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "60d6d138-5fe9-49c6-9a8d-ed3f1b70ee66")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "28abc8be-b07e-4da4-977e-473f3a2f39d5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -2.4 -1.138)
		(end 2.4 -1.138)
		(stroke
			(width 0.2032)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c2435fd3-fbe3-4d36-a202-8dea2c4ad6fd")
	)
	(fp_line
		(start -2.4 0.638)
		(end -2.4 -1.138)
		(stroke
			(width 0.2032)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "94eef341-c8fd-4ffb-a387-c4bc83b65e49")
	)
	(fp_line
		(start -2.4 1.138)
		(end -2.4 0.638)
		(stroke
			(width 0.2032)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fadcc1b4-e80f-4424-9299-2b805bd08d98")
	)
	(fp_line
		(start 2.4 -1.138)
		(end 2.4 0.638)
		(stroke
			(width 0.2032)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "65155d18-28f5-408c-b187-7766057421c7")
	)
	(fp_line
		(start 2.4 0.638)
		(end -2.4 0.638)
		(stroke
			(width 0.2032)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec490fac-7b8b-4a62-9fa5-0683eeb0be68")
	)
	(fp_line
		(start 2.4 0.638)
		(end 2.4 1.138)
		(stroke
			(width 0.2032)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2786a850-6999-42bc-ad04-ef25401252a2")
	)
	(fp_line
		(start 2.4 1.138)
		(end -2.4 1.138)
		(stroke
			(width 0.2032)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "82fae502-663c-45d4-9ee2-0b68269bac6d")
	)
	(fp_circle
		(center -2.032 0.254)
		(end -1.778 0.254)
		(stroke
			(width 0.127)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "1049f953-9b34-43e1-ad09-f14bcadf96dc")
	)
	(pad "1" smd rect
		(at -1.905 2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1adc15ad-3eda-4d78-9cd4-b5a7f65f9386")
	)
	(pad "2" smd rect
		(at -0.635 2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "83436f51-0358-4fed-b864-bfa196d32064")
	)
	(pad "3" smd rect
		(at 0.635 2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "3810a452-d0bb-48af-a9be-d537919e5dd2")
	)
	(pad "4" smd rect
		(at 1.905 2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "f113fb9f-69d6-4410-a210-40a290388e2c")
	)
	(pad "5" smd rect
		(at 1.905 -2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "bb8a9368-3e18-441a-afa5-1bbef416d6cf")
	)
	(pad "6" smd rect
		(at 0.635 -2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "37633175-30a0-46ea-bbd8-68ba3ad8af2a")
	)
	(pad "7" smd rect
		(at -0.635 -2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "954de067-78e8-429f-b2f6-26e6e1622e74")
	)
	(pad "8" smd rect
		(at -1.905 -2.6)
		(size 0.6 1.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "421d98a4-be8f-453d-bc98-d16564b2cc40")
	)
	(pad "P$1" smd rect
		(at 0 0)
		(size 4.9 2.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2ff8a209-0a2e-46f7-bb93-27e35dbbf11c")
	)
)
