(footprint "RCL_R0201"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "RESISTOR chip\n\nSource: http://www.vishay.com/docs/20008/dcrcw.pdf")
	(property "Reference" "REF**"
		(at -0.635 -0.635 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b196a37f-cdd1-496f-9cc4-e271d14146ce")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Value" "RCL_R0201"
		(at -0.635 1.905 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "88b7a79b-762b-4137-91fb-84e3c0b3dbc4")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c404ab8b-d16c-49fa-ab8d-14e68e937d12")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b192094b-363b-46eb-bc47-ed14f10978a1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "4778ce9d-bb6e-4afd-9fe0-934a10d17363")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_poly
		(pts
			(xy -0.15 0.15) (xy 0.15 0.15) (xy 0.15 -0.15) (xy -0.15 -0.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "a57ff5cd-b184-48cd-a852-dfcb232bb207")
	)
	(fp_poly
		(pts
			(xy -0.3 0.15) (xy -0.15 0.15) (xy -0.15 -0.15) (xy -0.3 -0.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.Fab")
		(uuid "28bf4b7b-2d4f-44e8-99e9-ccc8a16bf674")
	)
	(fp_poly
		(pts
			(xy 0.15 0.15) (xy 0.3 0.15) (xy 0.3 -0.15) (xy 0.15 -0.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.Fab")
		(uuid "e718ecb4-1f76-4cef-bc99-2ce5f32d2b9b")
	)
	(pad "1" smd rect
		(at -0.255 0)
		(size 0.28 0.43)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "711c73cb-18d1-4110-83d3-c27cb20a4a41")
	)
	(pad "2" smd rect
		(at 0.255 0)
		(size 0.28 0.43)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b53fadfc-1e22-4b28-acac-c1ad01279f21")
	)
)
