(footprint "DIODE_SMBJ"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "DO-214AA Modified J_BEND\n\nSource: www.rsonline.de .. SMBJ12/C/15/C/24/C/30/C/5.0/C/7.5/C Voltage Suppressor. Data Sheet")
	(property "Reference" "REF**"
		(at -1.905 -2.54 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f8c5d0fb-0143-4912-89e1-fa2541d782da")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Value" "DIODE_SMBJ"
		(at -1.905 3.81 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "59d980b3-bb0f-4808-a665-f7e5ad2c79cd")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3ac805dd-bf4b-4b50-858d-c520bc6347c4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "5d3b05cd-e0e1-44cd-8afd-39ad474020c4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "dd2239df-db78-42ee-97be-56e252443c40")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -2.24 -1.92)
		(end 2.24 -1.92)
		(stroke
			(width 0.1016)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "311fab42-feac-4487-a4ac-5c30dd8cc338")
	)
	(fp_line
		(start -0.8 -1.1)
		(end -0.8 1.1)
		(stroke
			(width 0.254)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3ed39a95-b23a-425b-9e5e-64b6f611f798")
	)
	(fp_line
		(start 2.24 1.92)
		(end -2.24 1.92)
		(stroke
			(width 0.1016)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6c52efd2-53a1-4fb6-b6de-1bea48dd0704")
	)
	(fp_poly
		(pts
			(xy 0.927 1.341431) (xy -1.024172 0) (xy 0.927 -1.341431)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.SilkS")
		(uuid "49bf0c46-b63f-4e0d-a2ea-59d735d59766")
	)
	(fp_line
		(start -2.24 1.92)
		(end -2.24 -1.92)
		(stroke
			(width 0.1016)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c05040fe-9c30-4e5a-b645-d0166f99414d")
	)
	(fp_line
		(start 2.24 -1.92)
		(end 2.24 1.92)
		(stroke
			(width 0.1016)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ffe79c48-dbe4-4304-a543-c64056d12bbb")
	)
	(fp_poly
		(pts
			(xy -2.8 1.1) (xy -2.25 1.1) (xy -2.25 -1.1) (xy -2.8 -1.1)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.Fab")
		(uuid "9956d30f-84de-4ea6-b6fe-61497971c610")
	)
	(fp_poly
		(pts
			(xy 2.25 1.1) (xy 2.8 1.1) (xy 2.8 -1.1) (xy 2.25 -1.1)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.Fab")
		(uuid "a4f59539-e544-46d2-b1ca-4bc13928feb6")
	)
	(pad "A" smd rect
		(at 2.04 0 180)
		(size 1.78 2.16)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "29e800df-7d57-434a-926b-5d358f11f95a")
	)
	(pad "C" smd rect
		(at -2.03 0)
		(size 1.78 2.16)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "924ca4f3-70d1-4f8f-9f3b-509468f56fbf")
	)
)
