(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "691321100002_EAGLE_WR-TBL_REV19A_691322110002"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 0.238 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.27 -2.54 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:691321100002_EAGLE_WR-TBL_REV19A_691322110002"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "WR-TBL Serie 3221 - 3.50mm Horizontal PCB Header, 2 Pins=>Code : Con_TBL_Pluggable_3.50_PCB_H_691322110002\n\nhttp://katalog.we-online.de/media/images/eican/Con_TBL_Pluggable_3.50_PCB_H_6913221100xx_pf2.jpg\n\nDetails see: http://katalog.we-online.de/en/em/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X http://katalog.we-online.de/en/em/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X\n\nCreated 2014-06-18, Karrer Zheng\n2014 (C) Würth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "691321100002_EAGLE_WR-TBL_REV19A_691322110002_1_0"
			(arc
				(start -1.651 -1.651)
				(mid -2.54 -2.54)
				(end -1.651 -3.429)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -1.651 0.889)
				(mid -2.54 0)
				(end -1.651 -0.889)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "ABS07W_ABS07-32.768KHZ-D-2-T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 1.016 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.54 -2.54 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:ABS07W_ABS07W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "32.768KHZ IoT OPTIMIZED SMD CRYSTAL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "ABS07W_ABS07-32.768KHZ-D-2-T_1_0"
			(polyline
				(pts
					(xy -2.54 0) (xy -1.016 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.016 1.778) (xy -1.016 -1.778)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.381 -1.524) (xy 0.381 -1.524)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.381 1.524) (xy -0.381 -1.524)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.381 -1.524) (xy 0.381 1.524)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.381 1.524) (xy -0.381 1.524)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 0) (xy 2.54 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.016 1.778) (xy 1.016 -1.778)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "1"
				(at -2.159 -1.143 0)
				(effects
					(font
						(size 0.8636 0.734)
					)
					(justify left bottom)
				)
			)
			(text "2"
				(at 1.524 -1.143 0)
				(effects
					(font
						(size 0.8636 0.734)
					)
					(justify left bottom)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 0)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 2.54 0 180)
				(length 0)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "ADP7118_ADP7118"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 10.16 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.54 -10.16 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:ADP7118_SOIC8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "ADP7118_ADP7118_1_0"
			(polyline
				(pts
					(xy -10.16 -7.62) (xy -10.16 7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -10.16 7.62) (xy 10.16 7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -7.62) (xy -10.16 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 7.62) (xy 10.16 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOUT2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SENSE/ADJ"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "EXP/PAD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "ADS1260_ADS1260"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 33.02 -35.56 90)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -15.24 15.24 90)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:ADS1260_VQFN-32"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "ADS126x Precision, 5-channel and 10-channel, 40-kSPS, 24-bit, delta-sigma ADCs with PGA and monitors"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "ADS1260_ADS1260_1_0"
			(polyline
				(pts
					(xy -12.7 -35.56) (xy 30.48 -35.56)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -12.7 20.32) (xy -12.7 -35.56)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 30.48 -35.56) (xy 30.48 20.32)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 30.48 20.32) (xy -12.7 20.32)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "AINCOM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "CS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 33.02 0 180)
				(length 2.54)
				(name "SCLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "DIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 33.02 7.62 180)
				(length 2.54)
				(name "DRDY"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "DOUT/DRDY"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "BYPASS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 -38.1 90)
				(length 2.54)
				(name "DGND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "DVDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "CLKIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 7.62 -38.1 90)
				(length 2.54)
				(name "NC-1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "CAPP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 10.16 -38.1 90)
				(length 2.54)
				(name "NC-2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 12.7 -38.1 90)
				(length 2.54)
				(name "NC-3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 15.24 -38.1 90)
				(length 2.54)
				(name "NC-4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 17.78 -38.1 90)
				(length 2.54)
				(name "NC-5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 20.32 -38.1 90)
				(length 2.54)
				(name "NC-6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 22.86 -38.1 90)
				(length 2.54)
				(name "NC-7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 25.4 -38.1 90)
				(length 2.54)
				(name "NC-8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin no_connect line
				(at 27.94 -38.1 90)
				(length 2.54)
				(name "NC-9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "AIN4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "AIN3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "CAPN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "AIN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "AIN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "AIN0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 -38.1 90)
				(length 2.54)
				(name "AVSS_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -5.08 -38.1 90)
				(length 2.54)
				(name "AVSS_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "AVSS_3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "AVSS_4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -7.62 22.86 270)
				(length 2.54)
				(name "AVDD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -10.16 -38.1 90)
				(length 2.54)
				(name "AVSS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "REFOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "PWDN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 33.02 12.7 180)
				(length 2.54)
				(name "RESET"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 33.02 15.24 180)
				(length 2.54)
				(name "START"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "A_CONN_PF2X5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at -2.54 8.255 0)
			(effects
				(font
					(size 2.032 1.7272)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.175 -10.16 0)
			(effects
				(font
					(size 2.032 1.7272)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:A_CONN_PF2X5"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "A_CONN_PF2X5_1_0"
			(circle
				(center -1.27 -5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 -2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 0)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 -6.985) (xy -3.175 6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 6.985) (xy 3.175 6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -5.08) (xy -1.905 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.905 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.905 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.905 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy -1.905 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 4.445) (xy -1.905 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 5.715) (xy -0.635 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 4.445) (xy -1.905 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 5.715) (xy -0.635 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 0) (xy 2.54 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 5.08) (xy 2.54 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 -6.985) (xy -3.175 -6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 6.985) (xy 3.175 -6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 -5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 -2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 0)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "10"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "9"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "A_CONN_PF2X5SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at -2.54 8.255 0)
			(effects
				(font
					(size 2.032 1.7272)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.175 -10.16 0)
			(effects
				(font
					(size 2.032 1.7272)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:A_CONN_PF2X5SMD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "A_CONN_PF2X5SMD_1_0"
			(circle
				(center -1.27 -5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 -2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 0)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 -6.985) (xy -3.175 6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 6.985) (xy 3.175 6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -5.08) (xy -1.905 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.905 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.905 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.905 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy -1.905 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 4.445) (xy -1.905 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 5.715) (xy -0.635 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 4.445) (xy -1.905 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 5.715) (xy -0.635 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 0) (xy 2.54 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 5.08) (xy 2.54 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 -6.985) (xy -3.175 -6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 6.985) (xy 3.175 -6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 -5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 -2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 0)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "10"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "9"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "A_CONN_PF2X5SMD1.27MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at -2.54 8.255 0)
			(effects
				(font
					(size 2.032 1.7272)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.175 -10.16 0)
			(effects
				(font
					(size 2.032 1.7272)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:A_CONN_PF2X5SMD50MIL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "A_CONN_PF2X5SMD1.27MM_1_0"
			(circle
				(center -1.27 -5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 -2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 0)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center -1.27 2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 -6.985) (xy -3.175 6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 6.985) (xy 3.175 6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -5.08) (xy -1.905 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.905 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.905 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.905 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy -1.905 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 4.445) (xy -1.905 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 5.715) (xy -0.635 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 4.445) (xy -1.905 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 5.715) (xy -0.635 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 0) (xy 2.54 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 5.08) (xy 2.54 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 -6.985) (xy -3.175 -6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 6.985) (xy 3.175 -6.985)
				)
				(stroke
					(width 0.508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 -5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 -2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 0)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 2.54)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 1.27 5.08)
				(radius 0.635)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "10"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "9"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "BOM_BOM-PART"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#BOM-PART"
			(at 1.27 -0.9525 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.27 -4.445 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "BOM ENTRY\n\nSpecial BOM entry-only specifier field."
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "BOM_BOM-PART_1_0"
			(polyline
				(pts
					(xy 0 -1.905) (xy 0 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 20.32 -1.905) (xy 0 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 20.32 -1.905) (xy 20.32 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 20.32 1.905) (xy 0 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "${DESC}"
				(at 1.27 3.175 0)
				(effects
					(font
						(size 1.778 1.5113)
					)
					(justify left bottom)
				)
			)
		)
	)
	(symbol "C247S_C247S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "OK"
			(at -10.16 -2.54 90)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 12.7 -2.54 90)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:C247S_SMD4"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "u Contact Form: C247S: 1A / C347S: 2A u Load Voltage: 80V Maximum u Operation LED Current: 3.0mA Maximum u Load Current: C247S: 1.25A Maximum / C347S: 1.0A Maximum u On-Resistance: 0.15Ω Typical u Output Capacitance: 190pF Typical u Low Off-State Leakage Current: 1.0μA Maximum"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "C247S_C247S_1_0"
			(polyline
				(pts
					(xy -7.62 -7.62) (xy -7.62 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -7.62 10.16) (xy -6.35 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.35 10.16) (xy -6.35 10.795)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.35 10.16) (xy -5.08 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -6.35 10.795) (xy -3.81 10.795)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 10.16) (xy -5.08 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 10.16) (xy -3.81 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 4.445) (xy -2.54 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 5.715) (xy -5.715 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 -8.255) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 -7.62) (xy -7.62 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 10.16) (xy 6.35 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 10.795) (xy -3.81 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 6.985) (xy -2.54 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -4.445) (xy -2.54 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 3.175) (xy -2.54 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 4.445) (xy -0.635 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.715) (xy -3.175 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.715) (xy -1.905 6.985)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 8.255) (xy -2.54 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 8.255) (xy 0 8.255)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 5.715) (xy -2.54 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 6.985) (xy -3.175 6.985)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -8.255) (xy -3.81 -8.255)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -7.62) (xy -2.54 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 -7.62) (xy -1.27 -8.255)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 -6.35) (xy 3.175 -4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 -4.445) (xy -2.54 -4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 -4.445) (xy -0.635 -6.35)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 -2.54) (xy -0.635 -4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 -0.635) (xy 0.635 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 8.255) (xy 0 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 8.255) (xy 2.54 8.255)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.635 1.27) (xy 1.905 -0.635)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.635 5.715) (xy -0.635 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.905 -0.635) (xy 3.175 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 8.255) (xy 2.54 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 8.255) (xy 5.08 8.255)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 -4.445) (xy -0.635 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 -4.445) (xy 3.175 -6.35)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 -4.445) (xy 5.08 -4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 -2.54) (xy 3.175 -4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 1.27) (xy 2.667 1.016)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 1.27) (xy 3.175 0.762)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 4.445) (xy 5.08 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.175 5.715) (xy 1.905 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -8.255) (xy 3.81 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy -1.27 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 4.445 6.985) (xy 5.715 6.985)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -7.62) (xy 3.81 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -4.445) (xy 5.08 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 3.175) (xy -2.54 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 4.445) (xy 5.08 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 4.445) (xy 6.985 4.445)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 5.715) (xy 4.445 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 5.715) (xy 4.445 6.985)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 8.255) (xy 5.08 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.715 5.715) (xy 5.08 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.715 6.985) (xy 5.08 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 -8.255) (xy 3.81 -8.255)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 -7.62) (xy 5.08 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 -7.62) (xy 6.35 -8.255)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 10.16) (xy 6.35 10.795)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 10.16) (xy 7.62 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 10.795) (xy 8.89 10.795)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.985 5.715) (xy 8.255 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 10.16) (xy 7.62 5.715)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 10.16) (xy 8.89 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 10.16) (xy 10.16 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 10.795) (xy 8.89 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -7.62) (xy 6.35 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 10.16) (xy 10.16 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 8.255)
				(radius 0.127)
				(stroke
					(width 1.27)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 2.54 8.255)
				(radius 0.127)
				(stroke
					(width 1.27)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 7.62 12.7 270)
				(length 2.54)
				(name "D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "D1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "CON-HARTING-ML_ML10"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SV"
			(at -3.81 8.382 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -10.16 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:CON-HARTING-ML_ML10"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "HARTING"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "CON-HARTING-ML_ML10_1_0"
			(polyline
				(pts
					(xy -3.81 7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -5.08) (xy -1.27 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.27 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.27 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy -1.27 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 2.54 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 5.08) (xy 2.54 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "10"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "9"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "CON-HARTING-ML_ML10-3M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SV"
			(at -3.81 8.382 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -10.16 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:CON-HARTING-ML_3M_10"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "HARTING"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "CON-HARTING-ML_ML10-3M_1_0"
			(polyline
				(pts
					(xy -3.81 7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -5.08) (xy -1.27 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.27 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.27 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy -1.27 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 2.54 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 5.08) (xy 2.54 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "10"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "9"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "CON-HARTING-ML_ML10-3ML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SV"
			(at -3.81 8.382 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -10.16 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:CON-HARTING-ML_3M_10L"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "HARTING"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "CON-HARTING-ML_ML10-3ML_1_0"
			(polyline
				(pts
					(xy -3.81 7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -5.08) (xy -1.27 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.27 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.27 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy -1.27 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 2.54 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 5.08) (xy 2.54 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "10"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "9"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "CON-HARTING-ML_ML10L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SV"
			(at -3.81 8.382 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -10.16 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:CON-HARTING-ML_ML10L"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "HARTING"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "CON-HARTING-ML_ML10L_1_0"
			(polyline
				(pts
					(xy -3.81 7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -5.08) (xy -1.27 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.27 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.27 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy -1.27 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 2.54 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 5.08) (xy 2.54 5.08)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy -3.81 -7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -7.62) (xy 3.81 7.62)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "10"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "9"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "CON-HARTING-ML_ML6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SV"
			(at -3.81 5.842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -7.62 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:CON-HARTING-ML_ML6"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "HARTING"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "CON-HARTING-ML_ML6_1_0"
			(polyline
				(pts
					(xy -3.81 5.08) (xy -3.81 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 5.08) (xy 3.81 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.27 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.27 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 2.54 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -5.08) (xy -3.81 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -5.08) (xy 3.81 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "CON-HARTING-ML_ML6L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SV"
			(at -3.81 5.842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -7.62 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:CON-HARTING-ML_ML6L"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "HARTING"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "CON-HARTING-ML_ML6L_1_0"
			(polyline
				(pts
					(xy -3.81 5.08) (xy -3.81 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 5.08) (xy 3.81 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.27 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 2.54) (xy -1.27 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 2.54 0)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 2.54) (xy 2.54 2.54)
				)
				(stroke
					(width 0.6096)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -5.08) (xy -3.81 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -5.08) (xy 3.81 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "DIODE_SUPPRESSOR-SMBG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.794 1.905 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -0.889 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:DIODE_SMBG"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Suppressor diode"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "DIODE_SUPPRESSOR-SMBG_1_0"
			(polyline
				(pts
					(xy -1.27 -1.27) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 1.27) (xy -1.27 0.635)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -1.27) (xy 1.27 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 1.27) (xy -1.27 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 1.27) (xy -1.27 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -1.27) (xy 0 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 1.27) (xy 0 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 1.905) (xy 1.27 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 0)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 0)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "DIODE_SUPPRESSOR-SMBJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.794 1.905 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -0.889 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:DIODE_SMBJ"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Suppressor diode"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "DIODE_SUPPRESSOR-SMBJ_1_0"
			(polyline
				(pts
					(xy -1.27 -1.27) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 1.27) (xy -1.27 0.635)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -1.27) (xy 1.27 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 1.27) (xy -1.27 -1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 1.27) (xy -1.27 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -1.27) (xy 0 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 1.27) (xy 0 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 1.905) (xy 1.27 1.27)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 0)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 0)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "EB-DIOS-M06_EB-DIOSM06"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at -5.08 12.7 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -5.08 -10.16 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:EB-DIOS-M06_PS_2-6"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "EB-DIOS M06 6-pol. Mini-DIN-Buchse, vollgeschirmt"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "EB-DIOS-M06_EB-DIOSM06_1_0"
			(polyline
				(pts
					(xy -5.08 -7.62) (xy 5.08 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 10.16) (xy -5.08 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 10.16) (xy -5.08 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 0 0)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 5.08)
				(name "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "EB-DIOS-M06_EB-DIOSM06_1_1"
			(pin power_in line
				(at -1.27 -10.16 90)
				(length 2.54)
				(name "A1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "A1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 1.27 -10.16 90)
				(length 2.54)
				(name "A2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "A2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 3.81 -10.16 90)
				(length 2.54)
				(name "A3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "A3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "FRAMES_A3L-LOC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FRAME"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "FRAME\n\nDIN A3, landscape with location and doc. field"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "FRAMES_A3L-LOC_1_0"
			(polyline
				(pts
					(xy 0 52.07) (xy 3.81 52.07)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 104.14) (xy 3.81 104.14)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 156.21) (xy 3.81 156.21)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 208.28) (xy 3.81 208.28)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 3.81) (xy 3.81 256.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 48.4188 0) (xy 48.4188 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 48.4188 256.54) (xy 48.4188 260.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 96.8375 0) (xy 96.8375 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 96.8375 256.54) (xy 96.8375 260.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 145.2563 0) (xy 145.2563 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 145.2563 256.54) (xy 145.2563 260.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 193.675 0) (xy 193.675 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 193.675 256.54) (xy 193.675 260.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 242.0938 0) (xy 242.0938 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 242.0938 256.54) (xy 242.0938 260.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 288.29 3.81) (xy 288.29 24.13)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 288.29 3.81) (xy 342.265 3.81)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 288.29 24.13) (xy 342.265 24.13)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 290.5125 0) (xy 290.5125 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 290.5125 256.54) (xy 290.5125 260.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 338.9313 0) (xy 338.9313 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 338.9313 256.54) (xy 338.9313 260.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 3.81) (xy 373.38 3.81)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 8.89) (xy 342.265 3.81)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 8.89) (xy 342.265 13.97)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 13.97) (xy 342.265 19.05)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 13.97) (xy 383.54 13.97)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 19.05) (xy 342.265 24.13)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 19.05) (xy 383.54 19.05)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 342.265 24.13) (xy 383.54 24.13)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 373.38 3.81) (xy 373.38 8.89)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 373.38 3.81) (xy 383.54 3.81)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 373.38 8.89) (xy 342.265 8.89)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 373.38 8.89) (xy 383.54 8.89)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 3.81) (xy 3.81 3.81)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 3.81) (xy 383.54 8.89)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 3.81) (xy 383.54 256.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 8.89) (xy 383.54 13.97)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 13.97) (xy 383.54 19.05)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 19.05) (xy 383.54 24.13)
				)
				(stroke
					(width 0.1016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 52.07) (xy 387.35 52.07)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 104.14) (xy 387.35 104.14)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 156.21) (xy 387.35 156.21)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 208.28) (xy 387.35 208.28)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 383.54 256.54) (xy 3.81 256.54)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 387.35 0) (xy 387.35 260.35) (xy 0 260.35) (xy 0 0)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "${#}/${##}"
				(at 357.505 5.08 0)
				(effects
					(font
						(size 2.54 2.159)
					)
					(justify left bottom)
				)
			)
			(text "${CURRENT_DATE}"
				(at 344.17 10.16 0)
				(effects
					(font
						(size 2.286 1.9431)
					)
					(justify left bottom)
				)
			)
			(text "${PROJECTNAME}"
				(at 344.17 15.24 0)
				(effects
					(font
						(size 2.54 2.159)
					)
					(justify left bottom)
				)
			)
			(text "1"
				(at 24.2094 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "1"
				(at 24.2094 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "2"
				(at 72.6281 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "2"
				(at 72.6281 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "3"
				(at 121.0469 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "3"
				(at 121.0469 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "4"
				(at 169.4656 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "4"
				(at 169.4656 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "5"
				(at 217.8844 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "5"
				(at 217.8844 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "6"
				(at 266.3031 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "6"
				(at 266.3031 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "7"
				(at 314.7219 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "7"
				(at 314.7219 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "8"
				(at 363.1406 1.905 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "8"
				(at 363.1406 258.445 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "A"
				(at 1.905 234.315 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "A"
				(at 385.445 234.315 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "B"
				(at 1.905 182.245 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "B"
				(at 385.445 182.245 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "C"
				(at 1.905 130.175 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "C"
				(at 385.445 130.175 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "D"
				(at 1.905 78.105 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "D"
				(at 385.445 78.105 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "E"
				(at 1.905 26.035 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "E"
				(at 385.445 26.035 0)
				(effects
					(font
						(size 2.54 2.286)
					)
				)
			)
			(text "Sheet:"
				(at 343.916 4.953 0)
				(effects
					(font
						(size 2.54 2.159)
					)
					(justify left bottom)
				)
			)
		)
	)
	(symbol "FUSE_SH32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "F"
			(at -3.81 1.397 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -2.921 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:FUSE_SH32"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "FUSE HOLDER\n\n6 x 32 mm, SH contact, SHH3N Schukat, 102071 Wickmann (Buerklin)"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "FUSE_SH32_1_0"
			(polyline
				(pts
					(xy -3.81 -0.762) (xy 3.81 -0.762)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 0.762) (xy -3.81 -0.762)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -0.762) (xy 3.81 0.762)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 0.762) (xy -3.81 0.762)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "1B"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1B"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "2B"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2B"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_6,4"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B6,4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND2.8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_2,8-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND2.8_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B2,8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND3.0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_3,0-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND3.0_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B3,0"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND3.2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_3,2-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND3.2_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B3,2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND3.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_3,3-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND3.3_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B3,3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND3.6"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_3,6-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND3.6_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B3,6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND4.1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_4,1-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND4.1_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B4,1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND4.3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_4,3-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND4.3_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B4,3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND4.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_4,5-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND4.5_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B4,5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND5.0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_5,0-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND5.0_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "HOLES_MOUNT-PAD-ROUND5.5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 2.794 0.5842 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.794 -2.4638 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:HOLES_5,5-PAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "MOUNTING PAD, round"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "HOLES_MOUNT-PAD-ROUND5.5_1_0"
			(arc
				(start -2.032 -0.254)
				(mid -1.448 -1.448)
				(end -0.254 -2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -0.254 2.032)
				(mid -1.448 1.448)
				(end -2.032 0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 0)
				(radius 1.524)
				(stroke
					(width 0.0508)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0.254 -2.032)
				(mid 1.448 -1.448)
				(end 2.032 -0.254)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.032 0.254)
				(mid 1.448 1.448)
				(end 0.254 2.032)
				(stroke
					(width 1.016)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -2.54 0 0)
				(length 2.54)
				(name "MOUNT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B6,4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "INA240_INA241"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 12.7 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.08 -10.16 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:INA240_SOT23-8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "INA240_INA241_1_0"
			(polyline
				(pts
					(xy -7.62 -5.08) (xy -7.62 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -7.62 10.16) (xy 10.16 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -5.08) (xy -7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 10.16) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "REF2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 12.7 270)
				(length 2.54)
				(name "VS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "REF1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "INA240_INA241DGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 12.7 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.08 -10.16 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:INA240_VSSOP"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "INA240_INA241DGK_1_0"
			(polyline
				(pts
					(xy -7.62 -5.08) (xy -7.62 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -7.62 10.16) (xy 10.16 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -5.08) (xy -7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 10.16) (xy 10.16 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "REF2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -5.08 -7.62 90)
				(length 2.54)
				(name "NC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 12.7 270)
				(length 2.54)
				(name "VS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "REF1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LED"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_SMARTLED-TTW"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LED_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A@1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C@1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LED-LUMILED"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LUMILED"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LED-LUMILED_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2+"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4-"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LED-LUMILED+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LUMILED+"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LED-LUMILED+_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2+"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4-"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LED10MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LED10MM"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LED10MM_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LED3MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LED3MM"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LED3MM_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LED5MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LED5MM"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LED5MM_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDB152"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_Q62902-B152"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDB152_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDB153"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_Q62902-B153"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDB153_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDB155"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_Q62902-B155"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDB155_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDB156"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_Q62902-B156"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDB156_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDCHIP-LED0603"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_CHIP-LED0603"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDCHIP-LED0603_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDCHIP-LED0805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_CHIP-LED0805"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDCHIP-LED0805_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDCHIPLED-0603-TTW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_CHIPLED-0603-TTW"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDCHIPLED-0603-TTW_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A@1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C@1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDCHIPLED_0603"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_CHIPLED_0603"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDCHIPLED_0603_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDCHIPLED_0805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_CHIPLED_0805"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDCHIPLED_0805_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDCHIPLED_1206"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_CHIPLED_1206"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDCHIPLED_1206_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDIRL80A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_IRL80A"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDIRL80A_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDKA-3528ASYC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_KA-3528ASYC"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDKA-3528ASYC_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDLD260"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LD260"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDLD260_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDLSU260"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LSU260"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDLSU260_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDLZR181"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LZR181"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDLZR181_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDMICRO-SIDELED"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_MICRO-SIDELED"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDMICRO-SIDELED_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDMINI-TOP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_OSRAM-MINI-TOP-LED"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDMINI-TOP_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDP-LCC-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_P-LCC-2"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDP-LCC-2_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDP-LCC-2-BACK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_P-LCC-2-TOPLED-RG"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDP-LCC-2-BACK_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDP-LCC-4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_P-LCC-4"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDP-LCC-4_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C@4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSFH480"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_SFH480"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSFH480_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSFH482"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_SFH482"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSFH482_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSIDELED"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_OSRAM-SIDELED"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSIDELED_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSMART-LED"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_SMART-LED"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSMART-LED_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSML0603"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_SML0603"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSML0603_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSML0805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_SML0805"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSML0805_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSML1206"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_SML1206"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSML1206_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSMT1206"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_1206"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSMT1206_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSQR2X5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_LED2X5"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSQR2X5_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDSQR5.7X3.2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_U57X32"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDSQR5.7X3.2_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "K"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "LED_LEDTOPLED-SANTANA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "LED"
			(at 3.556 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.715 -4.572 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:LED_MINI-TOPLED-SANTANA"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LED\n\nOSRAM:\n- CHIPLED\nLG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971 LH N974, LH R974\nLS Q976, LO Q976, LY Q976\nLO Q996\n- Hyper CHIPLED\nLW Q18S\nLB Q993, LB Q99A, LB R99A\n- SideLED\nLS A670, LO A670, LY A670, LG A670, LP A670\nLB A673, LV A673, LT A673, LW A673\nLH A674\nLY A675\nLS A676, LA A676, LO A676, LY A676, LW A676\nLS A679, LY A679, LG A679\n-  Hyper Micro SIDELED®\nLS Y876, LA Y876, LO Y876, LY Y876\nLT Y87S\n- SmartLED\nLW L88C, LW L88S\nLB L89C, LB L89S, LG L890\nLS L89K, LO L89K, LY L89K\nLS L896, LA L896, LO L896, LY L896\n- TOPLED\nLS T670, LO T670, LY T670, LG T670, LP T670\nLSG T670, LSP T670, LSY T670, LOP T670, LYG T670\nLG T671, LOG T671, LSG T671\nLB T673, LV T673, LT T673, LW T673\nLH T674\nLS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676\nLB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C\nLS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C\nLW T67C\nLS T679, LY T679, LG T679\nLS T770, LO T770, LY T770, LG T770, LP T770\nLB T773, LV T773, LT T773, LW T773\nLH T774\nLS E675, LA E675, LY E675, LS T675\nLS T776, LA T776, LO T776, LY T776, LB T776\nLHGB T686\nLT T68C, LB T68C\n- Hyper Mini TOPLED®\nLB M676\n- Mini TOPLED Santana®\nLG M470\nLS M47K, LO M47K, LY M47K\n\nSource: http://www.osram.convergy.de\n\nLUXEON:\n- LUMILED®\nLXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00\nLXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00\nLXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00\nLXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00\nLXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00\nLXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00\nLXK2-PH12-R00, LXK2-PH12-S00\nLXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00\n\nSource: www.luxeon.com\n\nKINGBRIGHT:\n\nKA-3528ASYC\nSource: www.kingbright.com"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "LED_LEDTOPLED-SANTANA_1_0"
			(polyline
				(pts
					(xy -2.032 -0.762) (xy -3.429 -2.159)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.905 -1.905) (xy -3.302 -3.302)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy -1.27 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.429 -2.159) (xy -3.048 -1.27) (xy -2.54 -1.778)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -3.302 -3.302) (xy -2.921 -2.413) (xy -2.413 -2.921)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "A"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "C"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "MAX6070_MAX6070"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -15.24 20.32 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -15.24 17.78 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:MAX6070_SOT23-6"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "MAX6070_MAX6070_1_0"
			(polyline
				(pts
					(xy -15.24 -17.78) (xy 17.78 -17.78)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -15.24 -2.54) (xy -10.16 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -15.24 10.16) (xy -15.24 -17.78)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -15.24 10.16) (xy -5.08 10.16)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -15.24 15.24) (xy -15.24 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -10.16 -5.08) (xy -10.16 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -10.16 -2.54) (xy -10.16 0)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -10.16 0) (xy -5.08 0)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 -15.24) (xy -5.08 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 -5.08) (xy -10.16 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 0) (xy -5.08 10.16)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 0) (xy 0 0)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 10.16) (xy 10.16 10.16)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -5.08) (xy -5.08 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 7.62)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 7.62) (xy 1.27 7.62)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -12.7) (xy 2.54 -12.7)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -5.08) (xy 1.27 -12.7)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 6.35) (xy 1.27 7.62)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 7.62) (xy 1.27 8.89)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 8.89) (xy 8.89 8.89)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -15.24) (xy -5.08 -15.24)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -15.24) (xy 10.16 -15.24)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -12.7) (xy 2.54 -15.24)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -12.7) (xy 3.81 -12.7)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -5.08) (xy 1.27 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -2.54) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -12.7) (xy 3.81 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 -5.08) (xy 2.54 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -5.08) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 2.54 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 5.08 5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 5.08) (xy 10.16 2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 6.35) (xy 1.27 6.35)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 7.62) (xy 8.89 6.35)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 7.62) (xy 17.78 7.62)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 8.89) (xy 8.89 7.62)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -15.24) (xy 10.16 -17.78)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -15.24) (xy 10.16 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -2.54) (xy 5.08 -5.08)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 2.54) (xy 15.24 0)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 10.16) (xy 10.16 2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.24 0) (xy 10.16 -2.54)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.24 0) (xy 17.78 0)
				)
				(stroke
					(width 0.127)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.78 -17.78) (xy 17.78 15.24)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 17.78 15.24) (xy -15.24 15.24)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "+"
				(at 6.35 -2.54 0)
				(effects
					(font
						(size 1.27 1.0795)
					)
					(justify left bottom)
				)
			)
			(text "-"
				(at 6.35 2.54 0)
				(effects
					(font
						(size 1.27 1.0795)
					)
					(justify left bottom)
				)
			)
			(text "Ref"
				(at -10.16 0 0)
				(effects
					(font
						(size 1.27 1.0795)
					)
					(justify left bottom)
				)
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "FILTER"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 10.16 -20.32 90)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "OUTS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "OUTF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "MAXIM_MAX22025"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 7.62 15.24 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 7.62 12.7 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:MAXIM_SO08-208"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Compact, Isolated, Half-Duplex RS-485/RS-422 Transceivers with AutoDirection Control"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "MAXIM_MAX22025_1_0"
			(polyline
				(pts
					(xy -12.7 -10.16) (xy -12.7 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -12.7 10.16) (xy 12.7 10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 12.7 -10.16) (xy -12.7 -10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 12.7 10.16) (xy 12.7 -10.16)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "RXD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "TXD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 5.08)
				(name "VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 5.08)
				(name "GNDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 5.08)
				(name "GNDB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "A"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 5.08)
				(name "VDDB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU01005"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C01005"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU01005_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025-024X044"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025-024X044"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025-024X044_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025-025X050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025-025X050"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025-025X050_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025-030X050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025-030X050"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025-030X050_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025-040X050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025-040X050"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025-040X050_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025-050X050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025-050X050"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025-050X050_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025-060X050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025-060X050"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025-060X050_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025_050-025X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025_050-025X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025_050-025X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025_050-035X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025_050-035X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025_050-035X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025_050-045X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025_050-045X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025_050-045X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU025_050-055X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025_050-055X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU025_050-055X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-024X044"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-024X044"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-024X044_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-025X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-025X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-025X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-030X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-030X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-030X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-035X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-035X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-035X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-045X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-045X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-045X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-050X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-050X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-050X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-055X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-055X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-055X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050-075X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050-075X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050-075X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU050H075X075"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C050H075X075"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU050H075X075_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU075-032X103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C075-032X103"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU075-032X103_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU075-042X103"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C075-042X103"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU075-042X103_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU075-052X106"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C075-052X106"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU075-052X106_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU075-063X106"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C075-063X106"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU075-063X106_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU102-043X133"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C102-043X133"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU102-043X133_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU102-054X133"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C102-054X133"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU102-054X133_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU102-064X133"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C102-064X133"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU102-064X133_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU102_152-062X184"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C102_152-062X184"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU102_152-062X184_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU150-054X183"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C150-054X183"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU150-054X183_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU150-064X183"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C150-064X183"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU150-064X183_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU150-072X183"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C150-072X183"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU150-072X183_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU150-084X183"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C150-084X183"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU150-084X183_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU150-091X182"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C150-091X182"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU150-091X182_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU225-062X268"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C225-062X268"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU225-062X268_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU225-074X268"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C225-074X268"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU225-074X268_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU225-087X268"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C225-087X268"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU225-087X268_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU225-108X268"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C225-108X268"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU225-108X268_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU225-113X268"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C225-113X268"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU225-113X268_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU275-093X316"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C275-093X316"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU275-093X316_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU275-113X316"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C275-113X316"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU275-113X316_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU275-134X316"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C275-134X316"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU275-134X316_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU275-154X316"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C275-154X316"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU275-154X316_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU275-173X316"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C275-173X316"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU275-173X316_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU275-205X316"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C275-205X316"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU275-205X316_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU325-137X374"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C325-137X374"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU325-137X374_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU325-162X374"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C325-162X374"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU325-162X374_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU325-182X374"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C325-182X374"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU325-182X374_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU375-155X418"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C375-155X418"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU375-155X418_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU375-192X418"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C375-192X418"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU375-192X418_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EU375-203X418"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C375-203X418"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EU375-203X418_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0201"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0201_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC025_050-024X070"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C025_050-024X070"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC025_050-024X070_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0402"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0402"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0402_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0402K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0402K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0402K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0504"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0504"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0504_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0603"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0603"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0603_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0603K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0603K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0603K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0805"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0805_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC0805K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C0805K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC0805K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1206"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1206"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1206_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1206K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1206K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1206K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1210"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1210"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1210_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1210K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1210K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1210K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1310"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1310"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1310_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1608"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1608"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1608_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1808"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1808"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1808_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1812"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1812"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1812_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1812K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1812K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1812K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1825"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1825"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1825_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC1825K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C1825K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC1825K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC2012"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C2012"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC2012_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC2220K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C2220K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC2220K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC2225K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C2225K"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC2225K_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC3216"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C3216"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC3216_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC3225"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C3225"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC3225_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC3640"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C3640"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC3640_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC4532"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C4532"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC4532_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUC4564"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_C4564"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUC4564_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_C-EUHPC0201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.524 0.381 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.524 -4.699 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_HPC0201"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "CAPACITOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_C-EUHPC0201_1_0"
			(rectangle
				(start -2.032 -2.032)
				(end 2.032 -1.524)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(rectangle
				(start -2.032 -1.016)
				(end 2.032 -0.508)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy 0 -2.032)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0) (xy 0 -0.508)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 2.54 270)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_01005"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R01005"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_01005_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0204/2V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0204V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0204/2V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0204/5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0204_5"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0204/5_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0204/7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0204_7"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0204/7_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0207/10"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0207_10"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0207/10_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0207/12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0207_12"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0207/12_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0207/15"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0207_15"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0207/15_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0207/2V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0207_2V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0207/2V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0207/5V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0207_5V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0207/5V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0207/7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0207_7"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0207/7_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0309/10"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0309_10"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0309/10_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0309/12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0309_12"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0309/12_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0309/V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0309V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0309/V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0411/12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0411_12"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0411/12_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0411/15"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0411_15"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0411/15_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0411/3V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0411V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0411/3V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0414/15"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0414_15"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0414/15_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0414/5V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0414V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0414/5V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0613/15"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_P0613_15"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0613/15_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0613/5V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_P0613V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0613/5V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0617/17"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0617_17"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0617/17_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0617/22"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0617_22"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0617/22_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0617/5V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0617V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0617/5V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0817/22"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_P0817_22"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0817/22_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0817/7V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_P0817V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0817/7V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0922/22"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0922_22"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0922/22_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_0922V"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_0922V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_0922V_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_1812X7R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_1812X7R"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_1812X7R_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M0805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M0805"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M0805_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M1206"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M1206"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M1206_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M1406"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M1406"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M1406_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M2012"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M2012"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M2012_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M2309"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M2309"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M2309_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M3216"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M3216"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M3216_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M3516"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M3516"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M3516_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_M5923"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_M5923"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_M5923_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_MELF0102AX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_MINI_MELF-0102AX"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_MELF0102AX_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_MELF0102R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_MINI_MELF-0102R"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_MELF0102R_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_MELF0102W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_MINI_MELF-0102W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_MELF0102W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_MELF0204R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_MINI_MELF-0204R"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_MELF0204R_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_MELF0204W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_MINI_MELF-0204W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_MELF0204W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_MELF0207R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_MINI_MELF-0207R"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_MELF0207R_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_MELF0207W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_MINI_MELF-0207W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_MELF0207W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_PRL1632"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_PRL1632"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_PRL1632_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R0201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R0201"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R0201_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R0402"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R0402"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R0402_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R0603"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R0603"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R0603_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R0805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R0805"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R0805_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R0805W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R0805W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R0805W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R1206"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R1206"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R1206_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R1206W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R1206W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R1206W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R1210"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R1210"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R1210_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R1210W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R1210W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R1210W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R1218"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R1218"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R1218_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R2010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R2010"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R2010_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R2010W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R2010W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R2010W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R2012"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R2012"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R2012_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R2012W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R2012W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R2012W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R2512"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R2512"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R2512_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R2512W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R2512W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R2512W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R3216"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R3216"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R3216_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R3216W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R3216W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R3216W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R3225"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R3225"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R3225_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R3225W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R3225W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R3225W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R4527"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R4527"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R4527_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R5025"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R5025"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R5025_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R5025W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R5025W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R5025W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R6332"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R6332"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R6332_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_R6332W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_R6332W"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_R6332W_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_RDH/15"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_RDH_15"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_RDH/15_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_V234/12"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_V234_12"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_V234/12_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_V235/17"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_V235_17"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_V235/17_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_V526-0"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_V526-0"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_V526-0_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_VMTA55"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_VMTA55"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_VMTA55_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_VMTB60"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_VMTB60"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_VMTB60_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_VTA52"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_VTA52"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_VTA52_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_VTA53"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_VTA53"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_VTA53_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_VTA54"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_VTA54"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_VTA54_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_VTA55"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_VTA55"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_VTA55_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_VTA56"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_VTA56"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_VTA56_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_WSC0001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_WSC0001"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_WSC0001_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_WSC0002"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_WSC0002"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_WSC0002_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_WSC01/2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_WSC01_2"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_WSC01/2_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_WSC2515"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_WSC2515"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_WSC2515_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_WSC4527"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_WSC4527"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_WSC4527_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "RCL_R-EU_WSC6927"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -3.81 1.4986 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -3.302 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:RCL_WSC6927"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "RESISTOR, European symbol"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "RCL_R-EU_WSC6927_1_0"
			(polyline
				(pts
					(xy -2.54 -0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 -0.889) (xy 2.54 -0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -0.889) (xy 2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 0.889) (xy -2.54 0.889)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "S08_MCP601OT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 3.175 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.54 -5.08 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:S08_SOT23-5"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single Op Amp 2.7V to 6.0V Single Supply CMOS\n\nSource: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "S08_MCP601OT_1_0"
			(polyline
				(pts
					(xy -5.08 -5.08) (xy 5.08 0)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 5.08) (xy -5.08 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 -2.54) (xy -3.175 -2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 2.54) (xy -3.175 2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 3.175) (xy -3.81 1.905)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy -5.08 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "V+"
				(at 1.27 3.175 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(text "V-"
				(at 1.27 -4.445 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "S08_MCP601P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 3.175 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.54 -5.08 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:S08_DIL08"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single Op Amp 2.7V to 6.0V Single Supply CMOS\n\nSource: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "S08_MCP601P_1_0"
			(polyline
				(pts
					(xy -5.08 -5.08) (xy 5.08 0)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 5.08) (xy -5.08 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 -2.54) (xy -3.175 -2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 2.54) (xy -3.175 2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 3.175) (xy -3.81 1.905)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy -5.08 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "V+"
				(at 1.27 3.175 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(text "V-"
				(at 1.27 -4.445 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "S08_MCP601R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 3.175 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.54 -5.08 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:S08_SOT23-5"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single Op Amp 2.7V to 6.0V Single Supply CMOS\n\nSource: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "S08_MCP601R_1_0"
			(polyline
				(pts
					(xy -5.08 -5.08) (xy 5.08 0)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 5.08) (xy -5.08 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 -2.54) (xy -3.175 -2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 2.54) (xy -3.175 2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 3.175) (xy -3.81 1.905)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy -5.08 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "V+"
				(at 1.27 3.175 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(text "V-"
				(at 1.27 -4.445 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "S08_MCP601SN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 3.175 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.54 -5.08 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:S08_SO08"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single Op Amp 2.7V to 6.0V Single Supply CMOS\n\nSource: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "S08_MCP601SN_1_0"
			(polyline
				(pts
					(xy -5.08 -5.08) (xy 5.08 0)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 5.08) (xy -5.08 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 -2.54) (xy -3.175 -2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 2.54) (xy -3.175 2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 3.175) (xy -3.81 1.905)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy -5.08 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "V+"
				(at 1.27 3.175 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(text "V-"
				(at 1.27 -4.445 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "S08_MCP601ST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 2.54 3.175 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 2.54 -5.08 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:S08_TSSOP8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Single Op Amp 2.7V to 6.0V Single Supply CMOS\n\nSource: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "S08_MCP601ST_1_0"
			(polyline
				(pts
					(xy -5.08 -5.08) (xy 5.08 0)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 5.08) (xy -5.08 -5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 -2.54) (xy -3.175 -2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 2.54) (xy -3.175 2.54)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 3.175) (xy -3.81 1.905)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 0) (xy -5.08 5.08)
				)
				(stroke
					(width 0.4064)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(text "V+"
				(at 1.27 3.175 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(text "V-"
				(at 1.27 -4.445 900)
				(effects
					(font
						(size 0.8128 0.6908)
					)
					(justify left bottom)
				)
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+IN"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 5.08)
				(name "V-"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 5.08)
				(name "V+"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "SIGNALCOMMUNICATIONS-(REV18E)_WE-LQFS_4818"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at -2.54 2.54 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -2.54 -2.54 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Footprint" "greenMeter_v3:SIGNALCOMMUNICATIONS-(REV18E)_WE-LQFS_48X8"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "WE-LQFS SMD Semishielded Tiny Power Inductor\n\nhttp://katalog.we-online.de/media/images/v2/Family_WE-LQFS_3818-4828.jpg\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-LQFS http://katalog.we-online.de/en/pbs/WE-LQFS\n\nCreated by Yingchun Shan\n2016 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SIGNALCOMMUNICATIONS-(REV18E)_WE-LQFS_4818_1_0"
			(arc
				(start -2.54 0)
				(mid -3.81 1.27)
				(end -5.08 0)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 0 0)
				(mid -1.27 1.27)
				(end -2.54 0)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 2.54 0)
				(mid 1.27 1.27)
				(end 0 0)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start 5.08 0)
				(mid 3.81 1.27)
				(end 2.54 0)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "SPARKFUN_GND"
		(power)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#GND"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -2.54 -2.54 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SUPPLY SYMBOL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SPARKFUN_GND_1_0"
			(polyline
				(pts
					(xy -1.905 0) (xy 1.905 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at 0 2.54 270)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "STM32G070_STM32G070KB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at 5.08 38.1 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 5.08 -35.56 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:STM32G070_LQFP32"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Arm® Cortex®-M0+ 32-bit MCU, 128 KB Flash, 36 KB RAM,   4x USART, timers, ADC, comm. I/Fs, 2.0-3.6V"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "STM32G070_STM32G070KB_1_0"
			(polyline
				(pts
					(xy -12.7 -33.02) (xy 15.24 -33.02)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -12.7 35.56) (xy -12.7 -33.02)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.24 -33.02) (xy 15.24 35.56)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 15.24 35.56) (xy -12.7 35.56)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PCP14-OSC32_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA11[PA9]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA12[PA10]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PA14-BOOT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PC15-OSC32_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PB6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PB7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PB8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD/VDDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS/VSSA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "NRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "SUPPLY1_+5V"
		(power)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#P+"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -2.54 -5.08 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SUPPLY SYMBOL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SUPPLY1_+5V_1_0"
			(polyline
				(pts
					(xy 0 0) (xy -1.27 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -1.905) (xy 0 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at 0 -2.54 90)
				(length 2.54)
				(name "+5V"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "SUPPLY1_GND"
		(power)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#GND"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -2.54 -2.54 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SUPPLY SYMBOL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SUPPLY1_GND_1_0"
			(polyline
				(pts
					(xy -1.905 0) (xy 1.905 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at 0 2.54 270)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "SUPPLY1_GND?{colon}1"
		(power)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#GND"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -2.54 -2.54 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SUPPLY SYMBOL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SUPPLY1_GND?{colon}1_1_0"
			(polyline
				(pts
					(xy -1.905 0) (xy 1.905 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at 0 2.54 270)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "SUPPLY1_VCC"
		(power)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#P+"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -2.54 -2.54 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SUPPLY SYMBOL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SUPPLY1_VCC_1_0"
			(polyline
				(pts
					(xy 0 0) (xy -1.27 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -1.905) (xy 0 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at 0 -2.54 90)
				(length 2.54)
				(name "VCC"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "SUPPLY1_VCC?{colon}1"
		(power)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#P+"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -2.54 -2.54 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SUPPLY SYMBOL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SUPPLY1_VCC?{colon}1_1_0"
			(polyline
				(pts
					(xy 0 0) (xy -1.27 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 -1.905) (xy 0 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at 0 -2.54 90)
				(length 2.54)
				(name "VCC"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "SUPPLY2_+UB"
		(power)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#SUPPLY"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at -1.905 3.175 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SUPPLY SYMBOL"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SUPPLY2_+UB_1_0"
			(polyline
				(pts
					(xy -0.635 1.27) (xy 0.635 1.27)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 0.635) (xy 0 1.905)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 1.27)
				(radius 1.27)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at 0 -2.54 90)
				(length 2.54)
				(name "+UB"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "SWITCH-OMRON_31-XX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "S"
			(at -6.35 -1.905 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 3.175 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:SWITCH-OMRON_B3F-31XX"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "OMRON SWITCH"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SWITCH-OMRON_31-XX_1_0"
			(polyline
				(pts
					(xy -4.445 -1.905) (xy -3.175 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 0) (xy -4.445 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 0) (xy -3.175 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 1.905) (xy -4.445 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -4.445 1.905) (xy -3.175 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 0) (xy -1.905 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 0) (xy -0.635 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 0) (xy -1.27 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -3.175) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 -2.54) (xy -0.635 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "P"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "S"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "SWITCH_LPV-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "S"
			(at -6.35 -1.905 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 2.54 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:SWITCH_LPV-1"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "TOGGLE SWITCH"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SWITCH_LPV-1_1_0"
			(polyline
				(pts
					(xy -5.08 1.905) (xy -3.81 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 0) (xy -3.81 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 0) (xy -1.905 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 1.905) (xy -3.81 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 1.905) (xy -2.54 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 0) (xy -0.762 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.762 0) (xy -0.254 -0.762)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.254 -0.762) (xy 0.254 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 1.27 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 0) (xy 0.635 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 1.905 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -3.175) (xy 2.54 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -1.905) (xy 0.635 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 5.08 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -3.175) (xy 7.62 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "O"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "P"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "S"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -5.08 90)
				(length 2.54)
				(name "B"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 270)
				(length 2.54)
				(name "B1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "SWITCH_LPV-15236WW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "S"
			(at -6.35 -1.905 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -3.81 2.54 90)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:SWITCH_5236WW"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "TOGGLE SWITCH"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "SWITCH_LPV-15236WW_1_0"
			(polyline
				(pts
					(xy -5.08 1.905) (xy -3.81 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 0) (xy -3.81 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 0) (xy -1.905 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 1.905) (xy -3.81 0)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 1.905) (xy -2.54 1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 0) (xy -0.762 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.762 0) (xy -0.254 -0.762)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.254 -0.762) (xy 0.254 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 1.27 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.254 0) (xy 0.635 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 0) (xy 1.905 0)
				)
				(stroke
					(width 0.1524)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -3.175) (xy 2.54 -1.905)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 2.54 -1.905) (xy 0.635 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 5.08 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -3.175) (xy 7.62 3.175)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "O"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "P"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 5.08 270)
				(length 2.54)
				(name "S"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 -5.08 90)
				(length 2.54)
				(name "B"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 7.62 5.08 270)
				(length 2.54)
				(name "B1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "B1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "TERMINALBLOCKS-(REV19A)_691322110004"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 1.27 0.238 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 1.27 -2.54 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:TERMINALBLOCKS-(REV19A)_691322110004"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "WR-TBL Serie 3221 - 3.50mm Horizontal PCB Header, 4 Pins=>Code : Con_TBL_Pluggable_3.50_PCB_H_691322110004\n\nhttp://katalog.we-online.de/media/images/eican/Con_TBL_Pluggable_3.50_PCB_H_6913221100xx_pf2.jpg\n\nDetails see: http://katalog.we-online.de/en/em/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X http://katalog.we-online.de/en/em/TBL_3_50_3221_HORIZONTAL_PCB_HEADER_69132211000X\n\nCreated 2014-06-18, Karrer Zheng\n2014 (C) Würth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "TERMINALBLOCKS-(REV19A)_691322110004_1_0"
			(arc
				(start -1.651 -1.651)
				(mid -2.54 -2.54)
				(end -1.651 -3.429)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -1.651 0.889)
				(mid -2.54 0)
				(end -1.651 -0.889)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -1.651 3.429)
				(mid -2.54 2.54)
				(end -1.651 1.651)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(arc
				(start -1.651 5.969)
				(mid -2.54 5.08)
				(end -1.651 4.191)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "TEXAS_LM5164"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -10.16 13.97 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -10.16 -17.78 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:TEXAS_SOIC8-POWERPAD"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "LM5164 100V Input, 1A Synchronous Buck DC/DC Converter With Ultra-low IQ"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "TEXAS_LM5164_1_0"
			(polyline
				(pts
					(xy -10.16 -15.24) (xy 10.16 -15.24)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -10.16 12.7) (xy -10.16 -15.24)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -15.24) (xy 10.16 12.7)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 12.7) (xy -10.16 12.7)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -12.7 0 0)
				(length 2.54)
				(name "RON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FB"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PG"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BOOST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -20.32 90)
				(length 5.08)
				(name "EXP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "P$1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "V-REG-3_LP2985M5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -7.62 8.28 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -7.62 -10.16 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:V-REG-3_SOT23-5_1"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "National Semiconductor Micropower Linear Regulator\n\n150mA regulated output, Vin 16V max., ultra-low dropout of 300mV @ 150mA, 1µA standby current, low noise"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "V-REG-3_LP2985M5_1_0"
			(polyline
				(pts
					(xy -7.62 -7.62) (xy 10.16 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -7.62 7.62) (xy -7.62 -7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 -7.62) (xy 10.16 7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 7.62) (xy -7.62 7.62)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VIN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "BYPASS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WIRE-TO-BOARD-(REV18A)_61200621721"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -17.272 0.762 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at -18.034 -2.54 0)
			(effects
				(font
					(size 1.778 1.5113)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WIRE-TO-BOARD-(REV18A)_61200621721"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WR-BHD 2.54mm Male Angled Box Header, 6 Pins=>Code : Con_WTB_BHD_2.54_Male_THT_WS_61200621721\nhttp://katalog.we-online.de/media/thumbs2/eican/thb_Con_WTB_BHD_2.54_Male_THT_WS_6120xx21721_pf2.jpg\n\nDetails see: http://katalog.we-online.de/en/em/612_0xx_217_21 http://katalog.we-online.de/en/em/612_0xx_217_21\n\nCreated 2014-06-05, Karrer Zheng\n2014 (C) Würth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WIRE-TO-BOARD-(REV18A)_61200621721_1_0"
			(polyline
				(pts
					(xy -7.62 -5.08) (xy 7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -7.62 5.08) (xy -7.62 -5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 -5.08) (xy 7.62 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 5.08) (xy -7.62 5.08)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at 5.08 10.16 270)
				(length 5.08)
				(name "6"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 5.08)
				(name "5"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 10.16 270)
				(length 5.08)
				(name "4"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 10.16 270)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331011452048"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331011452048"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331011452048_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331011452535"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331011452535"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331011452535_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331031271520"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331031271520"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331031271520_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331031321515"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331031321515"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331031321515_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331041402053"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331041402053"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331041402053_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331051472057"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331051472057"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331051472057_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331061603010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331061603010"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331061603010_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331081302025"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331081302025"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331081302025_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331141352540"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331141352540"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331141352540_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331151702562"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331151702562"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331151702562_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161452070"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161452070"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161452070_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161702513"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161702513"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161702513_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331171302030"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331171302030"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331171302030_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331171302035"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331171302035"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331171302035_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331211503040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331211503040"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331211503040_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331221602040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331221602040"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331221602040_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331236362553"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331236362553"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331236362553_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331246501860"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331246501860"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331246501860_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331256381840"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331256381840"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331256381840_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331265563040"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331265563040"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331265563040_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
	)
	(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331276483050"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "H"
			(at 0 3.81 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify bottom)
			)
		)
		(property "Value" ""
			(at -3.81 -5.08 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331276483050"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WE-SECF SMD EMI Contact Fingerr\n\nCharacteristics\n\nsuitable for automated placement\nMaterial: copper-beryllium (CuBe) gold-plated (Au)\nDifferent types and sizes available\nCorrossion-resistant\nWear-resistant\nHigh temperatures and mechanical weight have no influence on the excellent connection properties\nReliable solderability\nCustomized materials and platings are possible\nCustomized types and sizes are possible\n\nApplications\n\nContact between PCB's earth and housing\nLow Ω HF connection between earthing points of two PCB's lying upon each other\nEarthing of cooling units on high frequency\nConnection between signal and power supply of two PCB's on track\nConnection between PCB's and extern elements\n\nDetails see: http://katalog.we-online.de/en/pbs/WE-SECF? http://katalog.we-online.de/en/pbs/WE-SECF?\n\nUpdated  by  Ella Wu 2019-07-19\n2019 (C) Wurth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331276483050_1_0"
			(polyline
				(pts
					(xy 0 -2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 0 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin passive line
				(at -5.08 0 0)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 0 0)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WüRTH_WIRE-TO-BOARD_61900211021"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 7.62 0 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 7.62 -2.54 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WüRTH_WIRE-TO-BOARD_61900211021"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WR-WTB 2.54mm Right Angled Locking Header Bottom Locking, 2 Pins=>Code : Con_WTB_2.54_PCB_THT_61900211021\nhttp://katalog.we-online.de/media/thumbs2/eican/thb_Con_WTB_2.54_PCB_THT_6190xx11021_pf2.jpg\n\nDetails see: http://katalog.we-online.de/en/em/619_0xx_110_21 http://katalog.we-online.de/en/em/619_0xx_110_21\n\nCreated 2014-06-05, Karrer Zheng\n2014 (C) Würth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WüRTH_WIRE-TO-BOARD_61900211021_1_0"
			(polyline
				(pts
					(xy -5.08 -2.54) (xy -5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.08 2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy -5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -7.62 90)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
	(symbol "WüRTH_WIRE-TO-BOARD_61900311021"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "K"
			(at 7.62 0 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Value" ""
			(at 7.62 -2.54 0)
			(effects
				(font
					(size 1.27 1.0795)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "greenMeter_v3:WüRTH_WIRE-TO-BOARD_61900311021"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" " WR-WTB 2.54mm Right Angled Locking Header Bottom Locking, 3 Pins=>Code : Con_WTB_2.54_PCB_THT_61900311021\nhttp://katalog.we-online.de/media/thumbs2/eican/thb_Con_WTB_2.54_PCB_THT_6190xx11021_pf2.jpg\n\nDetails see: http://katalog.we-online.de/en/em/619_0xx_110_21 http://katalog.we-online.de/en/em/619_0xx_110_21\n\nCreated 2014-06-05, Karrer Zheng\n2014 (C) Würth Elektronik"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "WüRTH_WIRE-TO-BOARD_61900311021_1_0"
			(polyline
				(pts
					(xy -10.16 -2.54) (xy -10.16 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -10.16 2.54) (xy 5.08 2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 -2.54) (xy -10.16 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 2.54) (xy 5.08 -2.54)
				)
				(stroke
					(width 0.254)
					(type solid)
				)
				(fill
					(type none)
				)
			)
			(pin bidirectional line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -2.54 -7.62 90)
				(length 5.08)
				(name "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at -7.62 -7.62 90)
				(length 5.08)
				(name "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
)
