(footprint "WüRTH_WIRE-TO-BOARD_61900211021"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "WR-WTB 2.54mm Right Angled Locking Header Bottom Locking, 2 Pins")
	(property "Reference" "REF**"
		(at 4.785 6.05 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ae1bedeb-f4ac-468d-8ba5-9fecb23cdf6d")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Value" "WüRTH_WIRE-TO-BOARD_61900211021"
		(at 5.01 8.03 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "f99b6c9c-199e-483d-b018-21c33c915f77")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8673460b-ec2e-4762-8f42-4ddbd67d765b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "34e44bd4-4e0d-4d19-a1b1-7d8837aca1bb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "eb5537ed-9d47-4e33-bc6b-bb4641ec8d50")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -2.69 -0.93)
		(end 2.69 -0.93)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d108cc05-f6d8-4b94-9ee4-77587b12fb1a")
	)
	(fp_line
		(start -2.69 13.1)
		(end -2.69 -0.93)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ca9e1964-b629-44c6-8696-5966cee52186")
	)
	(fp_line
		(start 2.69 -0.93)
		(end 2.69 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ec6bd63b-e4be-466c-ab5f-475cf2883e26")
	)
	(fp_line
		(start 2.69 13.1)
		(end -2.69 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6f60df99-f03d-4d67-9d74-ca8ef4a6517d")
	)
	(fp_line
		(start -2.69 0)
		(end 2.69 0)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b5df74e0-e1cc-47e7-93b6-7a6b832683b3")
	)
	(fp_line
		(start -2.69 13.1)
		(end -2.69 0)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d3e1a54b-c851-48f9-ae2a-f9a76d87fe76")
	)
	(fp_line
		(start 2.69 0)
		(end 2.69 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f6c2bacf-f31c-452a-bfcb-903ab628af89")
	)
	(fp_line
		(start 2.69 13.1)
		(end -2.69 13.1)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "50b3955b-2242-4836-8e0d-b356e4acc75e")
	)
	(fp_text user "2"
		(at -1.905 0.635 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "1404cf69-acd4-49c3-b815-5593b89500d5")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(fp_text user "1"
		(at 0.635 0.635 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a2d1ea54-1c61-4556-947d-a7296e1b1adf")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(pad "1" thru_hole circle
		(at 1.27 0)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "d545a0a1-f1ef-44ab-b993-a5bd6f131959")
	)
	(pad "2" thru_hole circle
		(at -1.27 0)
		(size 1.508 1.508)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "4855dff0-cee3-4d08-a401-58469e216204")
	)
)
