(footprint "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161702513"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "WE-SECF SMD EMI Contact Finger\nSize: 1613\n7x2.5x13.2mm")
	(property "Reference" "REF**"
		(at 0 -2.79 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b00e7d02-7293-4eb6-9ebd-605199a379a5")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify bottom)
		)
	)
	(property "Value" "WURTH_EMC-COMPONENTS_WE-SECF_WE-SECF_331161702513"
		(at -3.41 3.96 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "96b42063-3cc5-4fe5-a7be-46a569d4eda8")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a7ecbccf-ac12-456d-8c96-9336cb533f3d")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "50f8d16c-f49e-4a8b-bfe5-0c9a8d144cb1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "465545a6-5586-4422-98c9-364ed3649caf")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -3.6 -1.35)
		(end -3.6 1.35)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "32716b42-1d03-427e-bbf5-0212b9b99383")
	)
	(fp_line
		(start -3.2 -1.35)
		(end -3.6 -1.35)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "9ec413bd-f601-4fc3-a995-3907138492d3")
	)
	(fp_line
		(start -3.2 1.35)
		(end -3.6 1.35)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d022018e-ce0d-4d61-ac8a-9f2bddf831f4")
	)
	(fp_line
		(start 3.3 -1.35)
		(end 3.6 -1.35)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5c8b2128-64c3-4051-acc6-fe945a10b677")
	)
	(fp_line
		(start 3.3 1.35)
		(end 3.6 1.35)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "057e443c-55d3-40ff-ba11-ecc8c4f75e92")
	)
	(fp_line
		(start 3.6 1.35)
		(end 3.6 -1.35)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cd0abbde-b1bb-4464-aeec-072b3a088a3a")
	)
	(fp_poly
		(pts
			(xy 5.3 2.3) (xy -5.3 2.3) (xy -5.3 -2.3) (xy 5.3 -2.3)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill solid)
		(layer "F.CrtYd")
		(uuid "87a7e1c4-7cb2-4278-9bc5-91d0f44da3e5")
	)
	(fp_line
		(start -3.5 -1.25)
		(end -3.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e30bdd72-ef9f-458e-8a26-e460702826bc")
	)
	(fp_line
		(start -3.5 -1.25)
		(end 3.5 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cc882cbd-9238-40ab-b84a-94695fa86a1d")
	)
	(fp_line
		(start 3.5 -1.25)
		(end 3.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "eda68e55-c374-4eee-be29-4d88bc4cd622")
	)
	(fp_line
		(start 3.5 1.25)
		(end -3.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c58c05eb-3881-43e4-9454-7da2137c4695")
	)
	(pad "1" smd rect
		(at 0.05 0)
		(size 5.8 2.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "f7efe348-8777-4915-ae92-7774c2a1afd6")
	)
)
