(footprint "STM32G070_LQFP32"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -5.6 3.2 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "1eec0cea-efb6-4b4c-893c-5f554d9f3ffe")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Value" "STM32G070_LQFP32"
		(at 6.8 3.2 90)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "b41b324f-6ebf-4523-bf00-15387a179a8c")
		(effects
			(font
				(size 1.1684 1.1684)
				(thickness 0.1016)
			)
			(justify left bottom)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8b5e5061-ec44-4129-b3ad-7fbe680c9032")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "48e485c9-f4e8-43e8-b155-ab37c49eb2c1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "60db848f-2715-4840-87db-315234282e11")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -3.5 -3.5)
		(end 3.5 -3.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "eed8dcbe-8d28-4ee1-b329-f6edbd7eb32c")
	)
	(fp_line
		(start -3.5 3.5)
		(end -3.5 -3.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e4aef7bc-b76b-4914-856f-db98169b4e7b")
	)
	(fp_line
		(start 3.5 -3.5)
		(end 3.5 3.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "408ef342-fb06-4a94-9485-ae45bf77325e")
	)
	(fp_line
		(start 3.5 3.5)
		(end -3.5 3.5)
		(stroke
			(width 0.127)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7b318887-632f-406b-8288-64b7f452fe4e")
	)
	(fp_circle
		(center -3.625 3.625)
		(end -3.5 3.625)
		(stroke
			(width 0.4064)
			(type solid)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "e3565a7e-c1a3-4c50-887d-d2c03eabd768")
	)
	(pad "1" smd rect
		(at -2.8 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "8c4f3b72-2d2c-42b1-b4dc-11723f8d5515")
	)
	(pad "2" smd rect
		(at -2 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "d6ef8471-3b8a-470a-b47d-095f7f97fd39")
	)
	(pad "3" smd rect
		(at -1.2 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "049ac2a4-ae9d-4811-ab2b-201d4c9c7a70")
	)
	(pad "4" smd rect
		(at -0.4 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "2efdc745-bf24-4e51-8293-0a46ae0ac504")
	)
	(pad "5" smd rect
		(at 0.4 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "fcd340d6-d05a-417f-9d8e-81eee7af429d")
	)
	(pad "6" smd rect
		(at 1.2 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "f262c7ac-9929-4a84-9817-da56606d791e")
	)
	(pad "7" smd rect
		(at 2 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "cf4f2b21-c05a-4ed2-afc8-94a385eb49ce")
	)
	(pad "8" smd rect
		(at 2.8 4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "e0f794a9-a522-4a6b-93aa-d326ae75d368")
	)
	(pad "9" smd rect
		(at 4.25 2.8 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "56b22ada-e359-48a9-9092-f10ecb1e1a95")
	)
	(pad "10" smd rect
		(at 4.25 2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "499bf2a0-9775-4dfa-b745-43d3fc2c56b9")
	)
	(pad "11" smd rect
		(at 4.25 1.2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "8de7fc1e-f066-4ea4-8d63-621143bd1438")
	)
	(pad "12" smd rect
		(at 4.25 0.4 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "dc115008-68af-4e67-b5a0-79da56888eb2")
	)
	(pad "13" smd rect
		(at 4.25 -0.4 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "95d4cc57-4bd3-4be2-84de-e4834ca717a2")
	)
	(pad "14" smd rect
		(at 4.25 -1.2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "048c0e96-dbaa-47d0-a26b-58403321a52b")
	)
	(pad "15" smd rect
		(at 4.25 -2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "57941a66-558b-4e60-b0c3-3ff055488b2f")
	)
	(pad "16" smd rect
		(at 4.25 -2.8 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5d5f342d-0e10-4e13-810d-f22a09b98499")
	)
	(pad "17" smd rect
		(at 2.8 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "d2968792-8163-427b-bb64-637dc0e717af")
	)
	(pad "18" smd rect
		(at 2 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "de9fb283-836f-4107-8a44-a5a1102b0f3c")
	)
	(pad "19" smd rect
		(at 1.2 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "27833d31-5ded-4991-b22f-6c8bf516f904")
	)
	(pad "20" smd rect
		(at 0.4 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "75187299-150e-4d72-837e-060ffa674e14")
	)
	(pad "21" smd rect
		(at -0.4 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "fde1f20e-f61c-40ad-9150-516c380002c0")
	)
	(pad "22" smd rect
		(at -1.2 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "5f1bb519-9008-4f77-a4a3-4e3c699053a6")
	)
	(pad "23" smd rect
		(at -2 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "1160b002-3658-425d-87d3-b66da1232562")
	)
	(pad "24" smd rect
		(at -2.8 -4.25 90)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "23e4382b-673b-4560-bb9a-5722f024bccd")
	)
	(pad "25" smd rect
		(at -4.25 -2.8 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "66a1dfcb-f645-44de-8a54-9c658f48e63c")
	)
	(pad "26" smd rect
		(at -4.25 -2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "f6635efe-9b38-48fb-8f4a-5dcca0fbfa23")
	)
	(pad "27" smd rect
		(at -4.25 -1.2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "a97c3448-13d6-4ff3-a7f4-19f58cb4af30")
	)
	(pad "28" smd rect
		(at -4.25 -0.4 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b7974482-ca75-4e22-9a56-bfd00de80f35")
	)
	(pad "29" smd rect
		(at -4.25 0.4 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "41b4a9cd-637e-4985-be39-255d80104dcb")
	)
	(pad "30" smd rect
		(at -4.25 1.2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "d2e105bd-9194-4612-a586-37b40570fb26")
	)
	(pad "31" smd rect
		(at -4.25 2 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "b30ccb5a-1347-446f-9c3d-b11b282491a2")
	)
	(pad "32" smd rect
		(at -4.25 2.8 180)
		(size 1.2 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
		(uuid "85cacbd7-ec48-4773-9dff-d57f65dafee3")
	)
)
