(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(uuid "dc58b905-d3ee-4405-a357-6dd5bf81d2a7")
	(paper "A4")
	(lib_symbols
		(symbol "Connector:Screw_Terminal_01x01"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "Screw_Terminal_01x01"
				(at 0 -2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Generic screw terminal, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "screw terminal"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "TerminalBlock*:*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "Screw_Terminal_01x01_1_1"
				(rectangle
					(start -1.27 1.27)
					(end 1.27 -1.27)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -0.5334 0.3302) (xy 0.3302 -0.508)
					)
					(stroke
						(width 0.1524)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.3556 0.508) (xy 0.508 -0.3302)
					)
					(stroke
						(width 0.1524)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 0)
					(radius 0.635)
					(stroke
						(width 0.1524)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Screw_Terminal_01x01")
		(at 100.33 82.55 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "59bf4b81-4900-4a9b-aa3a-7bd5d0bd9e06")
		(property "Reference" "J24"
			(at 99.314 84.836 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "Würth RedCube"
			(at 94.742 87.376 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "myWürthSHFU:WP-SHFU_7461098_HAL"
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2409261545_SAMZO-14580S0M5_C41416688.pdf"
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M5 SMD 6-PIN 150A"
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ECS Art#" "CON519"
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "HAN" " 14580S0"
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Voltage" ""
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Toleranz" ""
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Hersteller" "SAMZO "
			(at 100.33 82.55 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "1da798aa-b959-4c47-bf98-fd9958da4e2e")
		)
		(instances
			(project "greenSmartSwitch"
				(path "/bf1f8167-8e29-49cc-a467-dd9cc2c77246/5376d07f-3cc6-4cdc-8a97-d86082792d40"
					(reference "J24")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Screw_Terminal_01x01")
		(at 100.33 67.31 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "9e2a94b0-e014-4fd8-b31a-2e289526870b")
		(property "Reference" "J23"
			(at 115.57 67.3099 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "SAMZO 14580S0M5"
			(at 98.806 70.104 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "myChineseConnectors:14580S0M5"
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2409261545_SAMZO-14580S0M5_C41416688.pdf"
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M5 SMD 6-PIN 150A"
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ECS Art#" "CON519"
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "HAN" " 14580S0"
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Voltage" ""
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Toleranz" ""
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Hersteller" "SAMZO "
			(at 100.33 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "945a43c1-380d-41f4-a634-079cf5d6218d")
		)
		(instances
			(project "greenSmartSwitch"
				(path "/bf1f8167-8e29-49cc-a467-dd9cc2c77246/5376d07f-3cc6-4cdc-8a97-d86082792d40"
					(reference "J23")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Screw_Terminal_01x01")
		(at 116.84 68.58 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "b3d8b76d-7dd8-4014-a665-7d503ddf7569")
		(property "Reference" "J25"
			(at 117.856 70.866 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "SAMZO 14580S0M5"
			(at 134.62 65.532 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "myChineseConnectors:14580S0M5"
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2409261545_SAMZO-14580S0M5_C41416688.pdf"
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M5 SMD 6-PIN 150A"
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ECS Art#" "CON519"
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "HAN" " 14580S0"
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Voltage" ""
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Toleranz" ""
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Hersteller" "SAMZO "
			(at 116.84 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "72e8cfcb-0d3f-4651-8551-89fd8ba9acbe")
		)
		(instances
			(project "greenSmartSwitch"
				(path "/bf1f8167-8e29-49cc-a467-dd9cc2c77246/5376d07f-3cc6-4cdc-8a97-d86082792d40"
					(reference "J25")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Screw_Terminal_01x01")
		(at 116.84 83.82 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "c7f14d3a-6bc4-46f5-8828-6773d31b0eba")
		(property "Reference" "J26"
			(at 117.856 86.106 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "Würth RedCube"
			(at 134.62 80.772 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "myWürthSHFU:WP-SHFU_7461098_HAL"
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2409261545_SAMZO-14580S0M5_C41416688.pdf"
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SCHRAUBANSCHLUSS M5 SMD 6-PIN 150A"
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ECS Art#" "CON519"
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "HAN" " 14580S0"
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Voltage" ""
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Toleranz" ""
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Hersteller" "SAMZO "
			(at 116.84 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "4b536ea5-f994-4144-9c1b-c51bcd43db73")
		)
		(instances
			(project "greenSmartSwitch"
				(path "/bf1f8167-8e29-49cc-a467-dd9cc2c77246/5376d07f-3cc6-4cdc-8a97-d86082792d40"
					(reference "J26")
					(unit 1)
				)
			)
		)
	)
)
